IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Time stamp: "2022-02-22T18:31:26"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.40.95 - Exporter 21.2.1.0 - Alternate UI 21.2.1.0"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "lmmadruga" of Organization (no name given)
  Owner history of Person "lmmadruga" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1645172159 (2022-02-18T08:15:59Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Site" | long name "Site" | object type "Level:Level 1" | elevation -1000.
        contains 83 elements
          1 x IFCSLAB | type IFCSLABTYPE "ENEL-ES-SITE:ENEL-ES-SITE" | object type "ENEL-ES-SITE:ENEL-ES-SITE" | FLOOR | names: "ENEL-ES-SITE:ENEL-ES-SITE:808334" | material: "ENEL-I&N-GLOBAL-EARTH-Site"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EartingCable_B12P:_EartingCable_B12P" | object type "_EartingCable_B12P:_EartingCable_B12P" | names: "_EartingCable_B12P:_EartingCable_B12P:1450168" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_GroundStake:_GroundStake" | object type "_GroundStake:_GroundStake" | names: "_GroundStake:_GroundStake:1451978", "_GroundStake:_GroundStake:1452477" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-ZincGroundSystem": "ENEL-I&N-GLOBAL-TYPE-METAL-ZincGroundSystem")
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_GroundStake:_GroundStake" | object type "_GroundStake:_GroundStake" | names: "_GroundStake:_GroundStake:1452457", "_GroundStake:_GroundStake:1452476" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-ZincGroundSystem": "ENEL-I&N-GLOBAL-TYPE-METAL-ZincGroundSystem")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EartingCable_B12P:_EartingCable_B12P" | object type "_EartingCable_B12P:_EartingCable_B12P" | names: "_EartingCable_B12P:_EartingCable_B12P:1672485" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_lvConector:_lvConector" | object type "_lvConector:_lvConector" | names: "_lvConector:_lvConector:1682093", "_lvConector:_lvConector:1683437", "_lvConector:_lvConector:1683444" (+1 more) | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-Copper": "ENEL-I&N-GLOBAL-TYPE-METAL-Copper", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_TerminalCablePressure:_TerminalCablePressure" | object type "_TerminalCablePressure:_TerminalCablePressure" | names: "_TerminalCablePressure:_TerminalCablePressure:1739506", "_TerminalCablePressure:_TerminalCablePressure:1740634", "_TerminalCablePressure:_TerminalCablePressure:1752205" (+1 more) | material: "<Unnamed>"
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_CableClamp:_CableClamp" | object type "_CableClamp:_CableClamp" | names: "_CableClamp:_CableClamp:1741615", "_CableClamp:_CableClamp:1741627" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium"
          1 x IFCFURNITURE | type IFCFURNITURETYPE "_ArmarioBT:_ArmarioBT" | object type "_ArmarioBT:_ArmarioBT" | names: "_ArmarioBT:_ArmarioBT:1802756" | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium", "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-Copper": "ENEL-I&N-GLOBAL-TYPE-METAL-Copper")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | object type "_MVCableI5P:_MVCableI5P" | names: "_MVCableI5P:_MVCableI5P:1949064" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | object type "_MVCableI5P:_MVCableI5P" | names: "_MVCableI5P:_MVCableI5P:1949072" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | object type "_MVCableI5P:_MVCableI5P" | names: "_MVCableI5P:_MVCableI5P:1949080" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_SSAABox:_SSAABox" | object type "_SSAABox:_SSAABox" | names: "_SSAABox:_SSAABox:2000618" | material: constituents "MaterialConstituentSet" ("AYE_Plastic_White": "AYE_Plastic_White", "Aluminum, Anodized Red": "Aluminum, Anodized Red", "<Unnamed>": "<Unnamed>", "Acrylic": "Acrylic", "Laminate, Blue, Matte": "Laminate, Blue, Matte", "_RAL7044": "_RAL7044")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_CableSupport:_CableSupport" | object type "_CableSupport:_CableSupport" | names: "_CableSupport:_CableSupport:2011299" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_PAT:_PAT" | object type "_PAT:_PAT" | names: "_PAT:_PAT:2064176" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Boccola:_Boccola" | object type "_Boccola:_Boccola" | names: "_Boccola:_Boccola:2064183", "_Boccola:_Boccola:2064947" | material: "<Unnamed>"
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_PAT:_PAT" | object type "_PAT:_PAT" | names: "_PAT:_PAT:2064866", "_PAT:_PAT:2064975" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_PAT:_PAT" | object type "_PAT:_PAT" | names: "_PAT:_PAT:2064910" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_SideDoor:_SideDoor" | object type "_SideDoor:_SideDoor" | names: "_SideDoor:_SideDoor:2159198" | material: "AYE_Aluminiun_Connector"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_SideDoor:_SideDoor" | object type "_SideDoor:_SideDoor" | names: "_SideDoor:_SideDoor:2159199" | material: "AYE_Aluminiun_Connector"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_VanoBTDoor:_VanoBTDoor" | object type "_VanoBTDoor:_VanoBTDoor" | names: "_VanoBTDoor:_VanoBTDoor:2159200" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-SteelRAL7038": "ENEL-I&N-GLOBAL-TYPE-METAL-SteelRAL7038", "Textura Galnanizada": "Textura Galnanizada", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel", "<Unnamed>": "<Unnamed>", "AYE_Plastic_Black": "AYE_Plastic_Black", "AYE_Aluminiun_Connector": "AYE_Aluminiun_Connector")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_VanoMTDoor:_VanoMTDoor" | object type "_VanoMTDoor:_VanoMTDoor" | names: "_VanoMTDoor:_VanoMTDoor:2159201" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-SteelRAL7038": "ENEL-I&N-GLOBAL-TYPE-METAL-SteelRAL7038", "Textura Galnanizada": "Textura Galnanizada", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel", "AYE_Plastic_Black": "AYE_Plastic_Black", "<Unnamed>": "<Unnamed>", "AYE_Aluminiun_Connector": "AYE_Aluminiun_Connector")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_CableType1_I6P:_CableType1_I6P" | object type "_CableType1_I6P:_CableType1_I6P" | names: "_CableType1_I6P:_CableType1_I6P:2173868" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
          2 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "_Lamp:_Lamp" | object type "_Lamp:_Lamp" | names: "_Lamp:_Lamp:2312703", "_Lamp:_Lamp:2312830" | material: constituents "MaterialConstituentSet" ("Vetro": "Vetro", "<Unnamed>": "<Unnamed>")
          1 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "_Lamp:_Lamp" | object type "_Lamp:_Lamp" | names: "_Lamp:_Lamp:2312813" | material: constituents "MaterialConstituentSet" ("Vetro": "Vetro", "<Unnamed>": "<Unnamed>")
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_IsolateCoverConnector:_IsolateCoverConnector" | object type "_IsolateCoverConnector:_IsolateCoverConnector" | names: "_IsolateCoverConnector:_IsolateCoverConnector:2341697", "_IsolateCoverConnector:_IsolateCoverConnector:2342735", "_IsolateCoverConnector:_IsolateCoverConnector:2342747" (+1 more) | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Rubber"
          12 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_TerminalCablePressureWithScrew:_TerminalCablePressureWithScrew" | object type "_TerminalCablePressureWithScrew:_TerminalCablePressureWithScrew" | names: "_TerminalCablePressureWithScrew:_TerminalCablePressureWithScrew:2347409", "_TerminalCablePressureWithScrew:_TerminalCablePressureWithScrew:2347457", "_TerminalCablePressureWithScrew:_TerminalCablePressureWithScrew:2348506" (+9 more) | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2347555" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2348967" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2349662" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2351378" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2361997" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2362398" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2362922" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2363413" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2364041" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2451490" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_PuertaArmarioBTPeq:Peq" | object type "_PuertaArmarioBTPeq:Peq" | names: "_PuertaArmarioBTPeq:Peq:2498365" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_HoseBand:_HoseBand" | object type "_HoseBand:_HoseBand" | names: "_HoseBand:_HoseBand:2523759" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2583040" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | object type "_EarthingCable_B6P:_EarthingCable_B6P" | names: "_EarthingCable_B6P:_EarthingCable_B6P:2583108" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | object type "_MVCableI5P:_MVCableI5P" | names: "_MVCableI5P:_MVCableI5P:2608828" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | object type "_MVCableI5P:_MVCableI5P" | names: "_MVCableI5P:_MVCableI5P:2608835" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | object type "_MVCableI5P:_MVCableI5P" | names: "_MVCableI5P:_MVCableI5P:2608842" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_SinglePoleShunt:_SinglePoleShunt" | object type "_SinglePoleShunt:_SinglePoleShunt" | names: "_SinglePoleShunt:_SinglePoleShunt:2715117", "_SinglePoleShunt:_SinglePoleShunt:2715200", "_SinglePoleShunt:_SinglePoleShunt:2715228" (+1 more) | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast": "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast")
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_CablePin:_CablePin" | object type "_CablePin:_CablePin" | names: "_CablePin:_CablePin:2796923", "_CablePin:_CablePin:2796941", "_CablePin:_CablePin:2845467" (+3 more) | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin", "ENEL-I&N-GLOBAL-TYPE-METAL-Copper": "ENEL-I&N-GLOBAL-TYPE-METAL-Copper", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-PlasticRed": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-PlasticRed")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_SupportCisco1101:_SupportCisco1101" | object type "_SupportCisco1101:_SupportCisco1101" | names: "_SupportCisco1101:_SupportCisco1101:2829967" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Platen:_Platen" | object type "_Platen:_Platen" | names: "_Platen:_Platen:2946183" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Cable4Pole_I10P:_Cable4Pole_I10P" | object type "_Cable4Pole_I10P:_Cable4Pole_I10P" | names: "_Cable4Pole_I10P:_Cable4Pole_I10P:2955881" | material: "<Unnamed>"
      IFCBUILDINGSTOREY "Protection, Control, Metering" | long name "Protection, Control, Metering" | object type "Level:Level 1" | elevation -350.
        contains 27 elements
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "ENEL-IT-Concentrator:ENEL-IT-Concentrator" | object type "ENEL-IT-Concentrator:ENEL-IT-Concentrator" | names: "METER DATA CONCENTRATOR-ED_IT_510013_DMIAB000255_03" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Traslucent": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Traslucent", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOn": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOn", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedYellowOn": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedYellowOn", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOn": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOn", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOff": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOff", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedYellowOff": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedYellowOff", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff") | property sets: GLOB_CAT_MASTERDATA, LOC_TYPE_GR_CT, LOC_TYPE_MASTERDATA, LOC_TYPE_MATGROUP, TECH_DETAIL
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "ENEL-IT-UP2020PSBC:ENEL-IT-UP2020PSBC" | object type "ENEL-IT-UP2020PSBC:ENEL-IT-UP2020PSBC" | names: "MV/LV SUBSTATION REMOTE TERMINAL UNIT-ED_IT_510021_02" | material: constituents "MaterialConstituentSet" ("AYE_Plastic_Black": "AYE_Plastic_Black", "AYE_Plastic_White": "AYE_Plastic_White", "<Unnamed>": "<Unnamed>", "_RAL7044": "_RAL7044") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_MRTU_CT, SUBTYPE_MASTERDATA, TECH_DETAIL
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "ENEL-IT-UP2020UE8:ENEL-IT-UP2020UE8" | object type "ENEL-IT-UP2020UE8:ENEL-IT-UP2020UE8" | names: "MV/LV SUBSTATION REMOTE TERMINAL UNIT-ED_IT_510021_02" | material: constituents "MaterialConstituentSet" ("AYE_Plastic_White": "AYE_Plastic_White", "AYE_Plastic_Black": "AYE_Plastic_Black", "<Unnamed>": "<Unnamed>", "_RAL7044": "_RAL7044") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_MRTU_CT, SUBTYPE_MASTERDATA, TECH_DETAIL
          1 x IFCELECTRICFLOWSTORAGEDEVICE | type IFCELECTRICFLOWSTORAGEDEVICETYPE "ENEL-IT-Battery:ENEL-IT-Battery" | object type "ENEL-IT-Battery:ENEL-IT-Battery" | names: "SEALED LEAD ACCUMULATOR BATTERY-ED_IT_162068_00" | material: constituents "MaterialConstituentSet" ("AYE_Plastic_Black": "AYE_Plastic_Black", "_AceroGalvanizado": "_AceroGalvanizado", "_PlásticoRojo": "_PlásticoRojo", "AYE_Plastic_White": "AYE_Plastic_White") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_BA_CT, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, SUBTYPE_BA_CT, SUBTYPE_MASTERDATA
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "ENEL-IT-RGDM:ENEL-IT-RGDM" | object type "ENEL-IT-RGDM:ENEL-IT-RGDM" | names: "ADVANCED FAULT PASSAGE INDICATOR-ED_IT_160077_01" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-Rubber": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Rubber", "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast": "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOn": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOn", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_RGA_CT, SUBTYPE_MASTERDATA, SUBTYPE_RGA_CT
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "ENEL-IT-AntennaType2:ENEL-IT-AntennaType2" | object type "ENEL-IT-AntennaType2:ENEL-IT-AntennaType2" | names: "ANTENNA ESTERNA OMNIDIREZIONALE-SP_ED_IT_480002_00" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium") | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "ENEL-IT-AntennaType1:ENEL-IT-AntennaType1" | object type "ENEL-IT-AntennaType1:ENEL-IT-AntennaType1" | names: "Antenna esterna omnidirezionale larga ba-SP_ED_IT_510002_02" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium") | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "ENEL-IT-Modem:ENEL-IT-Modem" | object type "ENEL-IT-Modem:ENEL-IT-Modem" | names: "ROUTER-ED_IT_470002_DMIAC000159_01" | material: constituents "MaterialConstituentSet" ("Laminate, Ivory, Matte": "Laminate, Ivory, Matte", "Laminate, Black": "Laminate, Black") | property sets: GLOB_CAT_MASTERDATA, LOC_TYPE_MASTERDATA, LOC_TYPE_MATGROUP, LOC_TYPE_RS_CT, OEM_RS_CT, OEM_RS_CT_IT
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "ENEL-IT-CISCOIR1101:ENEL-IT-CISCOIR1101" | object type "ENEL-IT-CISCOIR1101:ENEL-IT-CISCOIR1101" | names: "ROUTER-ED_IT_480015_IR1101_00" | material: constituents "MaterialConstituentSet" ("AYE_Plastic_Black": "AYE_Plastic_Black", "Iron, Ductile": "Iron, Ductile", "Acrylic": "Acrylic", "Laminate, Green, Matte": "Laminate, Green, Matte", "Laminate, Yellow, Matte": "Laminate, Yellow, Matte", "<Unnamed>": "<Unnamed>") | property sets: GLOB_CAT_MASTERDATA, LOC_TYPE_MASTERDATA, LOC_TYPE_MATGROUP, LOC_TYPE_RS_CT, OEM_RS_CT, OEM_RS_CT_IT
          1 x IFCFLOWMETER | type IFCFLOWMETERTYPE "ENEL-IT-EnergyMeter:ENEL-IT-EnergyMeter" | object type "ENEL-IT-EnergyMeter:ENEL-IT-EnergyMeter" | names: "THREE PHASE SEMI-DIRECT CONNECTION METER-ED_IT_516225_DMIAB000253_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin", "<Unnamed>": "<Unnamed>") | property sets: GLOB_CAT_MASTERDATA, LOC_TYPE_MASTERDATA, LOC_TYPE_MATGROUP, LOC_TYPE_XR_CT, OEM_XR_CT, TECH_DETAIL
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "ENEL-IT-Adaptatore:ENEL-IT-Adaptatore" | object type "ENEL-IT-Adaptatore:ENEL-IT-Adaptatore" | names: "Adattatore FSL per RGDM – DY1051/2-SP_ED_IT_140090_01" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin") | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | object type "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I10PDYN:ENEL-IT-ColigamentoUP_I10PDYN" | object type "ENEL-IT-ColigamentoUP_I10PDYN:ENEL-IT-ColigamentoUP_I10PDYN" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | object type "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | object type "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | object type "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I50P:ENEL-IT-ColigamentoUP_I50P" | object type "ENEL-IT-ColigamentoUP_I50P:ENEL-IT-ColigamentoUP_I50P" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I50P:ENEL-IT-ColigamentoUP_I50P" | object type "ENEL-IT-ColigamentoUP_I50P:ENEL-IT-ColigamentoUP_I50P" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | object type "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | object type "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | object type "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | object type "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | names: "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCOVERING | type IFCCOVERINGTYPE "ENEL-IT-EnergyMeterBase:ENEL-IT-EnergyMeterBase" | object type "ENEL-IT-EnergyMeterBase:ENEL-IT-EnergyMeterBase" | names: "Basetta per l'installazione del contatore per Bilancio Energia tipo GESIS-SP_ED_IT_280011_02" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCPROTECTIVEDEVICE | type IFCPROTECTIVEDEVICETYPE "ENEL-IT-ColigamentoGesis:ENEL-IT-ColigamentoGesis" | object type "ENEL-IT-ColigamentoGesis:ENEL-IT-ColigamentoGesis" | names: "Presa per il collegamento del contatore per Bilancio Energia tipo GESIS-SP_ED_IT_280176_04" | material: "<Unnamed>" | property sets: SP_MASTERDATA, TECH_DETAIL
          3 x IFCFLOWMETER | type IFCFLOWMETERTYPE "ENEL-IT-CurrentTransformerToroidal:ENEL-IT-CurrentTransformerToroidal" | object type "ENEL-IT-CurrentTransformerToroidal:ENEL-IT-CurrentTransformerToroidal" | names: "THREE PHASE SEMI-DIRECT CONNECTION METER-ED_IT_530002_DMI031003_03" | material: "<Unnamed>" | property sets: GLOB_CAT_MASTERDATA, LOC_TYPE_MASTERDATA, LOC_TYPE_MATGROUP, LOC_TYPE_XR_CT, OEM_XR_CT, TECH_DETAIL
      IFCBUILDINGSTOREY "Cabin" | long name "Cabin" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCCOVERING | type IFCCOVERINGTYPE "ENEL-IT-Minibox:ENEL-IT-Minibox" | object type "ENEL-IT-Minibox:ENEL-IT-Minibox" | names: "PREFABRICATED CONCRETE CABINET-ED_IT_227481_DG2081_05" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper" | property sets: GLOB_CAT_MASTERDATA, LOC_TYPE_MASTERDATA, LOC_TYPE_MATGROUP, LOC_TYPE_XM_CT, OEM_XM_CT, TECH_DETAIL
      IFCBUILDINGSTOREY "LV Section" | long name "LV Section" | object type "Level:Level 1" | elevation 1000.
        contains 58 elements
          2 x IFCFURNITURE | type IFCFURNITURETYPE "ENEL-IT-SwitchboardSupport:ENEL-IT-SwitchboardSupport" | object type "ENEL-IT-SwitchboardSupport:ENEL-IT-SwitchboardSupport" | names: "TELAIO ACCIAIO SUPPORTO QUADRO BT-SP_ED_IT_160650_03" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Grey2" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | object type "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | object type "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | object type "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | object type "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | object type "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | object type "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | object type "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | object type "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          2 x IFCCABLEFITTING | type IFCCABLEFITTINGTYPE "ENEL-IT-TerminaEarthinglCablePressure:ENEL-IT-TerminaEarthinglCablePressure" | object type "ENEL-IT-TerminaEarthinglCablePressure:ENEL-IT-TerminaEarthinglCablePressure" | names: "CAPOCORDA IN LEGA D'ALLUMINIO CON VITE DI SERRAGGIO-SP_ED_IT_210562_03" | material: "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | object type "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | names: "LV UNDERGROUND CABLE-ED_IT_330304_05" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XCL_CT, SUBTYPE_MASTERDATA, SUBTYPE_XCL_CT
          16 x IFCCABLEFITTING | type IFCCABLEFITTINGTYPE "ENEL-IT-LVIsolateCableClamp:ENEL-IT-LVIsolateCableClamp" | object type "ENEL-IT-LVIsolateCableClamp:ENEL-IT-LVIsolateCableClamp" | names: "MORS PERF CTO CAV BT EA0138/3UE-SP_ED_IT_852122_06" | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-SteelConnection": "ENEL-I&N-GLOBAL-TYPE-METAL-SteelConnection", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Polimeric": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Polimeric", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel") | property sets: SP_MASTERDATA, TECH_DETAIL
          2 x IFCPROTECTIVEDEVICE | type IFCPROTECTIVEDEVICETYPE "ENEL-IT-Switchboard:ENEL-IT-Switchboard" | object type "ENEL-IT-Switchboard:ENEL-IT-Switchboard" | names: "SECONDARY SUBSTATIONS LV SWITCHBOARDS-ED_IT_160125_01" | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel", "ENEL-I&N-GLOBAL-METAL-Brass": "ENEL-I&N-GLOBAL-METAL-Brass", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Grey": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Grey", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XQ_CT, SUBTYPE_MASTERDATA, SUBTYPE_XQ_CT
          8 x IFCCABLEFITTING | type IFCCABLEFITTINGTYPE "ENEL-IT-Conector1Fouri:ENEL-IT-Conector1Fouri" | object type "ENEL-IT-Conector1Fouri:ENEL-IT-Conector1Fouri" | names: "CAPOCORDA COMPR DIR. 150/13,0BT-SP_ED_IT_210580_01" | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel") | property sets: SP_MASTERDATA, TECH_DETAIL
          4 x IFCPROTECTIVEDEVICE | type IFCPROTECTIVEDEVICETYPE "ENEL-IT-MotorizedCircuitBreakerType4:ENEL-IT-MotorizedCircuitBreakerType4" | object type "ENEL-IT-MotorizedCircuitBreakerType4:ENEL-IT-MotorizedCircuitBreakerType4" | names: "LV MCCB CIRCUIT BREAKER-ED_IT_131118_00" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-Grey": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Grey", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Red": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Red", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Black": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Black", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-White": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-White", "ENEL-I&N-GLOBAL-METAL-Brass": "ENEL-I&N-GLOBAL-METAL-Brass") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XH_CT, OEM_XH_CT, SUBTYPE_MASTERDATA
      IFCBUILDINGSTOREY "Transformer" | long name "Transformer" | object type "Level:Level 1" | elevation 1500.
        contains 4 elements
          1 x IFCTRANSFORMER | type IFCTRANSFORMERTYPE "ENEL-IT-Transformer400KVA:ENEL-IT-Transformer400KVA" | object type "ENEL-IT-Transformer400KVA:ENEL-IT-Transformer400KVA" | names: "MV/LV TRANSFORMER-ED_IT_113638_03" | material: constituents "MaterialConstituentSet" ("AYE_Steel_Galvanized": "AYE_Steel_Galvanized", "AYE_Plastic_Black": "AYE_Plastic_Black", "AYE_Metal_LacqueredWhite": "AYE_Metal_LacqueredWhite", "<Unnamed>": "<Unnamed>", "AYE_Ceramic_Isolator": "AYE_Ceramic_Isolator", "AYE_Aluminiun_Connector": "AYE_Aluminiun_Connector", "AYE_Aluminiun_Conductor": "AYE_Aluminiun_Conductor", "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast": "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_MB_CT, OEM_MB_CT, SUBTYPE_MASTERDATA
          3 x IFCPROTECTIVEDEVICE | type IFCPROTECTIVEDEVICETYPE "ENEL-IT-Fuse63A:ENEL-IT-Fuse63A" | object type "ENEL-IT-Fuse63A:ENEL-IT-Fuse63A" | names: "CURRENT LIMITING FUSE-LINK-ED_IT_172544_DY561_02" | material: "<Unnamed>" | property sets: GLOB_CAT_MASTERDATA, LOC_TYPE_MASTERDATA, LOC_TYPE_MATGROUP, LOC_TYPE_XFMC_CT, OEM_XFMC_CT, TECH_DETAIL
      IFCBUILDINGSTOREY "MV Section" | long name "MV Section" | object type "Level:Level 1" | elevation 2000.
        contains 22 elements
          1 x IFCPROTECTIVEDEVICE | type IFCPROTECTIVEDEVICETYPE "ENEL-IT-Switchgear2L1T:ENEL-IT-Switchgear2L1T" | object type "ENEL-IT-Switchgear2L1T:ENEL-IT-Switchgear2L1T" | names: "SECONDARY SUBSTATION GAS INSULATED MV SWITCHGEAR / CIRCUIT BREAKER-ED_IT_140050_00" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronCast": "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast", "AYE_Plastic_Black": "AYE_Plastic_Black", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium", "<Unnamed>": "<Unnamed>", "AYE_Steel_Box": "AYE_Steel_Box", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff") | property sets: GLOB_CAT_MASTERDATA, GLOB_TYPE_MASTERDATA, GLOB_TYPE_MATGROUP, GLOB_TYPE_XZM_CT, OEM_XZM_CT, SUBTYPE_MASTERDATA
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamento_I10P:ENEL-IT-KITCollegamento_I10P" | object type "ENEL-IT-KITCollegamento_I10P:ENEL-IT-KITCollegamento_I10P" | names: "KIT COLLEGAMENTO TRAFO MT-SP_ED_IT_279713_04" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableRED" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamento_I10P:ENEL-IT-KITCollegamento_I10P" | object type "ENEL-IT-KITCollegamento_I10P:ENEL-IT-KITCollegamento_I10P" | names: "KIT COLLEGAMENTO TRAFO MT-SP_ED_IT_279713_04" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableRED" | property sets: SP_MASTERDATA, TECH_DETAIL
          1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamento_I10P:ENEL-IT-KITCollegamento_I10P" | object type "ENEL-IT-KITCollegamento_I10P:ENEL-IT-KITCollegamento_I10P" | names: "KIT COLLEGAMENTO TRAFO MT-SP_ED_IT_279713_04" | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableRED" | property sets: SP_MASTERDATA, TECH_DETAIL
          3 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamentoConnectionTT:ENEL-IT-KITCollegamentoConnectionTT" | object type "ENEL-IT-KITCollegamentoConnectionTT:ENEL-IT-KITCollegamentoConnectionTT" | names: "KIT COLLEGAMENTO TRAFO MT-SP_ED_IT_279713_04" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel", "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-SteelConnection": "ENEL-I&N-GLOBAL-TYPE-METAL-SteelConnection") | property sets: SP_MASTERDATA, TECH_DETAIL
          3 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamentoConnectionSTRAFO:ENEL-IT-KITCollegamentoConnectionSTRAFO" | object type "ENEL-IT-KITCollegamentoConnectionSTRAFO:ENEL-IT-KITCollegamentoConnectionSTRAFO" | names: "KIT COLLEGAMENTO TRAFO MT-SP_ED_IT_279713_04" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-CERAMIC-IsolatorRAL9011": "ENEL-I&N-GLOBAL-TYPE-CERAMIC-IsolatorRAL9011", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium") | property sets: SP_MASTERDATA, TECH_DETAIL
          6 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamentoConnectionSLinea:ENEL-IT-KITCollegamentoConnectionSLinea" | object type "ENEL-IT-KITCollegamentoConnectionSLinea:ENEL-IT-KITCollegamentoConnectionSLinea" | names: "KIT COLLEGAMENTO TRAFO MT-SP_ED_IT_279713_04" | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-CERAMIC-IsolatorRAL9011": "ENEL-I&N-GLOBAL-TYPE-CERAMIC-IsolatorRAL9011", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium") | property sets: SP_MASTERDATA, TECH_DETAIL
          6 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "ENEL-IT-CableHole:ENEL-IT-CableHole" | object type "ENEL-IT-CableHole:ENEL-IT-CableHole" | names: "PASSACAVO STAGNO PER CABINE SECONDARIE-SP_ED_IT_226721_01" | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel") | property sets: SP_MASTERDATA, TECH_DETAIL

Types
  IFCSLABTYPE "ENEL-ES-SITE:ENEL-ES-SITE" | FLOOR | 1 occurrence | material: "ENEL-I&N-GLOBAL-EARTH-Site"
  IFCBUILDINGELEMENTPROXYTYPE "_EartingCable_B12P:_EartingCable_B12P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_GroundStake:_GroundStake" | 2 occurrences | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-ZincGroundSystem": "ENEL-I&N-GLOBAL-TYPE-METAL-ZincGroundSystem")
  IFCBUILDINGELEMENTPROXYTYPE "_GroundStake:_GroundStake" | 2 occurrences | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-ZincGroundSystem": "ENEL-I&N-GLOBAL-TYPE-METAL-ZincGroundSystem")
  IFCBUILDINGELEMENTPROXYTYPE "_EartingCable_B12P:_EartingCable_B12P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_lvConector:_lvConector" | 4 occurrences | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-Copper": "ENEL-I&N-GLOBAL-TYPE-METAL-Copper", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCBUILDINGELEMENTPROXYTYPE "_TerminalCablePressure:_TerminalCablePressure" | 4 occurrences | material: "<Unnamed>"
  IFCBUILDINGELEMENTPROXYTYPE "_CableClamp:_CableClamp" | 2 occurrences | material: "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium"
  IFCFURNITURETYPE "_ArmarioBT:_ArmarioBT" | 1 occurrence | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium", "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-Copper": "ENEL-I&N-GLOBAL-TYPE-METAL-Copper")
  IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCBUILDINGELEMENTPROXYTYPE "_SSAABox:_SSAABox" | 1 occurrence | material: constituents "MaterialConstituentSet" ("AYE_Plastic_White": "AYE_Plastic_White", "Aluminum, Anodized Red": "Aluminum, Anodized Red", "<Unnamed>": "<Unnamed>", "Acrylic": "Acrylic", "Laminate, Blue, Matte": "Laminate, Blue, Matte", "_RAL7044": "_RAL7044")
  IFCBUILDINGELEMENTPROXYTYPE "_CableSupport:_CableSupport" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel"
  IFCBUILDINGELEMENTPROXYTYPE "_PAT:_PAT" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_Boccola:_Boccola" | 2 occurrences | material: "<Unnamed>"
  IFCBUILDINGELEMENTPROXYTYPE "_PAT:_PAT" | 2 occurrences | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_PAT:_PAT" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_SideDoor:_SideDoor" | 1 occurrence | material: "AYE_Aluminiun_Connector"
  IFCBUILDINGELEMENTPROXYTYPE "_SideDoor:_SideDoor" | 1 occurrence | material: "AYE_Aluminiun_Connector"
  IFCBUILDINGELEMENTPROXYTYPE "_VanoBTDoor:_VanoBTDoor" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-SteelRAL7038": "ENEL-I&N-GLOBAL-TYPE-METAL-SteelRAL7038", "Textura Galnanizada": "Textura Galnanizada", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel", "<Unnamed>": "<Unnamed>", "AYE_Plastic_Black": "AYE_Plastic_Black", "AYE_Aluminiun_Connector": "AYE_Aluminiun_Connector")
  IFCBUILDINGELEMENTPROXYTYPE "_VanoMTDoor:_VanoMTDoor" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-SteelRAL7038": "ENEL-I&N-GLOBAL-TYPE-METAL-SteelRAL7038", "Textura Galnanizada": "Textura Galnanizada", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel", "AYE_Plastic_Black": "AYE_Plastic_Black", "<Unnamed>": "<Unnamed>", "AYE_Aluminiun_Connector": "AYE_Aluminiun_Connector")
  IFCBUILDINGELEMENTPROXYTYPE "_CableType1_I6P:_CableType1_I6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCLIGHTFIXTURETYPE "_Lamp:_Lamp" | 2 occurrences | material: constituents "MaterialConstituentSet" ("Vetro": "Vetro", "<Unnamed>": "<Unnamed>")
  IFCLIGHTFIXTURETYPE "_Lamp:_Lamp" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Vetro": "Vetro", "<Unnamed>": "<Unnamed>")
  IFCBUILDINGELEMENTPROXYTYPE "_IsolateCoverConnector:_IsolateCoverConnector" | 4 occurrences | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Rubber"
  IFCBUILDINGELEMENTPROXYTYPE "_TerminalCablePressureWithScrew:_TerminalCablePressureWithScrew" | 12 occurrences | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel")
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_PuertaArmarioBTPeq:Peq" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium"
  IFCBUILDINGELEMENTPROXYTYPE "_HoseBand:_HoseBand" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_EarthingCable_B6P:_EarthingCable_B6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCBUILDINGELEMENTPROXYTYPE "_MVCableI5P:_MVCableI5P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCBUILDINGELEMENTPROXYTYPE "_SinglePoleShunt:_SinglePoleShunt" | 4 occurrences | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast": "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast")
  IFCBUILDINGELEMENTPROXYTYPE "_CablePin:_CablePin" | 6 occurrences | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin", "ENEL-I&N-GLOBAL-TYPE-METAL-Copper": "ENEL-I&N-GLOBAL-TYPE-METAL-Copper", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-PlasticRed": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-PlasticRed")
  IFCBUILDINGELEMENTPROXYTYPE "_SupportCisco1101:_SupportCisco1101" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast"
  IFCBUILDINGELEMENTPROXYTYPE "_Platen:_Platen" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-METAL-Copper"
  IFCBUILDINGELEMENTPROXYTYPE "_Cable4Pole_I10P:_Cable4Pole_I10P" | 1 occurrence | material: "<Unnamed>"
  IFCELECTRICAPPLIANCETYPE "ENEL-IT-Concentrator:ENEL-IT-Concentrator" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Traslucent": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Traslucent", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOn": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOn", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedYellowOn": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedYellowOn", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOn": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOn", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOff": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOff", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedYellowOff": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedYellowOff", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff")
  IFCELECTRICAPPLIANCETYPE "ENEL-IT-UP2020PSBC:ENEL-IT-UP2020PSBC" | 1 occurrence | material: constituents "MaterialConstituentSet" ("AYE_Plastic_Black": "AYE_Plastic_Black", "AYE_Plastic_White": "AYE_Plastic_White", "<Unnamed>": "<Unnamed>", "_RAL7044": "_RAL7044")
  IFCELECTRICAPPLIANCETYPE "ENEL-IT-UP2020UE8:ENEL-IT-UP2020UE8" | 1 occurrence | material: constituents "MaterialConstituentSet" ("AYE_Plastic_White": "AYE_Plastic_White", "AYE_Plastic_Black": "AYE_Plastic_Black", "<Unnamed>": "<Unnamed>", "_RAL7044": "_RAL7044")
  IFCELECTRICFLOWSTORAGEDEVICETYPE "ENEL-IT-Battery:ENEL-IT-Battery" | 1 occurrence | material: constituents "MaterialConstituentSet" ("AYE_Plastic_Black": "AYE_Plastic_Black", "_AceroGalvanizado": "_AceroGalvanizado", "_PlásticoRojo": "_PlásticoRojo", "AYE_Plastic_White": "AYE_Plastic_White")
  IFCELECTRICAPPLIANCETYPE "ENEL-IT-RGDM:ENEL-IT-RGDM" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-Rubber": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Rubber", "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast": "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOn": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedRedOn", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin")
  IFCELECTRICAPPLIANCETYPE "ENEL-IT-AntennaType2:ENEL-IT-AntennaType2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium")
  IFCELECTRICAPPLIANCETYPE "ENEL-IT-AntennaType1:ENEL-IT-AntennaType1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium")
  IFCELECTRICAPPLIANCETYPE "ENEL-IT-Modem:ENEL-IT-Modem" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Laminate, Ivory, Matte": "Laminate, Ivory, Matte", "Laminate, Black": "Laminate, Black")
  IFCELECTRICAPPLIANCETYPE "ENEL-IT-CISCOIR1101:ENEL-IT-CISCOIR1101" | 1 occurrence | material: constituents "MaterialConstituentSet" ("AYE_Plastic_Black": "AYE_Plastic_Black", "Iron, Ductile": "Iron, Ductile", "Acrylic": "Acrylic", "Laminate, Green, Matte": "Laminate, Green, Matte", "Laminate, Yellow, Matte": "Laminate, Yellow, Matte", "<Unnamed>": "<Unnamed>")
  IFCFLOWMETERTYPE "ENEL-IT-EnergyMeter:ENEL-IT-EnergyMeter" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin", "<Unnamed>": "<Unnamed>")
  IFCELECTRICAPPLIANCETYPE "ENEL-IT-Adaptatore:ENEL-IT-Adaptatore" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin")
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I10PDYN:ENEL-IT-ColigamentoUP_I10PDYN" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I6P:ENEL-IT-ColigamentoUP_I6P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I50P:ENEL-IT-ColigamentoUP_I50P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I50P:ENEL-IT-ColigamentoUP_I50P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCCABLESEGMENTTYPE "ENEL-IT-ColigamentoUP_I10P:ENEL-IT-ColigamentoUP_I10P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray"
  IFCCOVERINGTYPE "ENEL-IT-EnergyMeterBase:ENEL-IT-EnergyMeterBase" | 1 occurrence
  IFCPROTECTIVEDEVICETYPE "ENEL-IT-ColigamentoGesis:ENEL-IT-ColigamentoGesis" | 1 occurrence | material: "<Unnamed>"
  IFCFLOWMETERTYPE "ENEL-IT-CurrentTransformerToroidal:ENEL-IT-CurrentTransformerToroidal" | 3 occurrences | material: "<Unnamed>"
  IFCCOVERINGTYPE "ENEL-IT-Minibox:ENEL-IT-Minibox" | 1 occurrence
  IFCFURNITURETYPE "ENEL-IT-SwitchboardSupport:ENEL-IT-SwitchboardSupport" | 2 occurrences | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Grey2"
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I10P:ENEL-IT-Cable_I10P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLEFITTINGTYPE "ENEL-IT-TerminaEarthinglCablePressure:ENEL-IT-TerminaEarthinglCablePressure" | 2 occurrences | material: "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel"
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLESEGMENTTYPE "ENEL-IT-Cable_I7P:ENEL-IT-Cable_I7P" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableGray", "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable": "ENEL-I&N-GLOBAL-TYPE-METAL-AluminiumCable")
  IFCCABLEFITTINGTYPE "ENEL-IT-LVIsolateCableClamp:ENEL-IT-LVIsolateCableClamp" | 16 occurrences | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-SteelConnection": "ENEL-I&N-GLOBAL-TYPE-METAL-SteelConnection", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Polimeric": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Polimeric", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel")
  IFCPROTECTIVEDEVICETYPE "ENEL-IT-Switchboard:ENEL-IT-Switchboard" | 2 occurrences | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel", "ENEL-I&N-GLOBAL-METAL-Brass": "ENEL-I&N-GLOBAL-METAL-Brass", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Grey": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Grey", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Resin")
  IFCCABLEFITTINGTYPE "ENEL-IT-Conector1Fouri:ENEL-IT-Conector1Fouri" | 8 occurrences | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel")
  IFCPROTECTIVEDEVICETYPE "ENEL-IT-MotorizedCircuitBreakerType4:ENEL-IT-MotorizedCircuitBreakerType4" | 4 occurrences | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-PLASTIC-Grey": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Grey", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Red": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Red", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Black": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-Black", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-White": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-White", "ENEL-I&N-GLOBAL-METAL-Brass": "ENEL-I&N-GLOBAL-METAL-Brass")
  IFCTRANSFORMERTYPE "ENEL-IT-Transformer400KVA:ENEL-IT-Transformer400KVA" | 1 occurrence | material: constituents "MaterialConstituentSet" ("AYE_Steel_Galvanized": "AYE_Steel_Galvanized", "AYE_Plastic_Black": "AYE_Plastic_Black", "AYE_Metal_LacqueredWhite": "AYE_Metal_LacqueredWhite", "<Unnamed>": "<Unnamed>", "AYE_Ceramic_Isolator": "AYE_Ceramic_Isolator", "AYE_Aluminiun_Connector": "AYE_Aluminiun_Connector", "AYE_Aluminiun_Conductor": "AYE_Aluminiun_Conductor", "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast": "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast")
  IFCPROTECTIVEDEVICETYPE "ENEL-IT-Fuse63A:ENEL-IT-Fuse63A" | 3 occurrences | material: "<Unnamed>"
  IFCPROTECTIVEDEVICETYPE "ENEL-IT-Switchgear2L1T:ENEL-IT-Switchgear2L1T" | 1 occurrence | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-IronCast": "ENEL-I&N-GLOBAL-TYPE-METAL-IronCast", "AYE_Plastic_Black": "AYE_Plastic_Black", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium", "<Unnamed>": "<Unnamed>", "AYE_Steel_Box": "AYE_Steel_Box", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-BirdLife", "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff": "ENEL-I&N-GLOBAL-TYPE-PLASTIC-LedGreenOff")
  IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamento_I10P:ENEL-IT-KITCollegamento_I10P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableRED"
  IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamento_I10P:ENEL-IT-KITCollegamento_I10P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableRED"
  IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamento_I10P:ENEL-IT-KITCollegamento_I10P" | 1 occurrence | material: "ENEL-I&N-GLOBAL-TYPE-PLASTIC-IsolateCableRED"
  IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamentoConnectionTT:ENEL-IT-KITCollegamentoConnectionTT" | 3 occurrences | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel", "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew": "ENEL-I&N-GLOBAL-TYPE-METAL-IronScrew", "ENEL-I&N-GLOBAL-TYPE-METAL-SteelConnection": "ENEL-I&N-GLOBAL-TYPE-METAL-SteelConnection")
  IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamentoConnectionSTRAFO:ENEL-IT-KITCollegamentoConnectionSTRAFO" | 3 occurrences | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-CERAMIC-IsolatorRAL9011": "ENEL-I&N-GLOBAL-TYPE-CERAMIC-IsolatorRAL9011", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium")
  IFCCABLESEGMENTTYPE "ENEL-IT-KITCollegamentoConnectionSLinea:ENEL-IT-KITCollegamentoConnectionSLinea" | 6 occurrences | material: constituents "MaterialConstituentSet" ("ENEL-I&N-GLOBAL-TYPE-CERAMIC-IsolatorRAL9011": "ENEL-I&N-GLOBAL-TYPE-CERAMIC-IsolatorRAL9011", "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium": "ENEL-I&N-GLOBAL-TYPE-METAL-CastAluminium")
  IFCCABLECARRIERSEGMENTTYPE "ENEL-IT-CableHole:ENEL-IT-CableHole" | 6 occurrences | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel": "ENEL-I&N-GLOBAL-TYPE-METAL-StainlessSteel")

Property sets
  GLOB_CAT_MASTERDATA | properties | on 24 objects (24 IFCCABLESEGMENT)
    GLOB_CAT_MASTERDATA__GLOB_CAT_CODE = "XCL" (IFCTEXT)
    GLOB_CAT_MASTERDATA__GLOB_CAT_DESC = "LV UNDERGROUND CABLE" (IFCTEXT)
    GLOB_CAT_MASTERDATA__IS_MULTIBAY = TRUE (IFCBOOLEAN)
    GLOB_CAT_MASTERDATA__SCHEME = "[N] Network" (IFCTEXT)
    GLOB_CAT_MASTERDATA__TYPE = "[C] Component" (IFCTEXT)
  GLOB_CAT_MASTERDATA | properties | on 4 objects (4 IFCFLOWMETER)
    GLOB_CAT_MASTERDATA__GLOB_CAT_CODE = "XR" (IFCTEXT)
    GLOB_CAT_MASTERDATA__GLOB_CAT_DESC = "THREE PHASE SEMI-DIRECT CONNECTION METER" (IFCTEXT)
    GLOB_CAT_MASTERDATA__IS_MULTIBAY = TRUE (IFCBOOLEAN)
    GLOB_CAT_MASTERDATA__SCHEME = "[N] Network" (IFCTEXT)
    GLOB_CAT_MASTERDATA__TYPE = "[C] Component" (IFCTEXT)
  GLOB_CAT_MASTERDATA | properties | on 4 objects (4 IFCPROTECTIVEDEVICE)
    GLOB_CAT_MASTERDATA__GLOB_CAT_CODE = "XH" (IFCTEXT)
    GLOB_CAT_MASTERDATA__GLOB_CAT_DESC = "LV MCCB CIRCUIT BREAKER" (IFCTEXT)
    GLOB_CAT_MASTERDATA__IS_MULTIBAY = TRUE (IFCBOOLEAN)
    GLOB_CAT_MASTERDATA__SCHEME = "[N] Network" (IFCTEXT)
    GLOB_CAT_MASTERDATA__TYPE = "[C] Component" (IFCTEXT)
  GLOB_CAT_MASTERDATA | properties | on 3 objects (3 IFCPROTECTIVEDEVICE)
    GLOB_CAT_MASTERDATA__GLOB_CAT_CODE = "_XFMC" (IFCTEXT)
    GLOB_CAT_MASTERDATA__GLOB_CAT_DESC = "CURRENT LIMITING FUSE-LINK" (IFCTEXT)
    GLOB_CAT_MASTERDATA__IS_MULTIBAY = TRUE (IFCBOOLEAN)
    GLOB_CAT_MASTERDATA__SCHEME = "[N] Network" (IFCTEXT)
    GLOB_CAT_MASTERDATA__TYPE = "[C] Component" (IFCTEXT)
  GLOB_CAT_MASTERDATA | properties | on 2 objects (2 IFCELECTRICAPPLIANCE)
    GLOB_CAT_MASTERDATA__GLOB_CAT_CODE = "_MRTU" (IFCTEXT)
    GLOB_CAT_MASTERDATA__GLOB_CAT_DESC = "MV/LV SUBSTATION REMOTE TERMINAL UNIT" (IFCTEXT)
    GLOB_CAT_MASTERDATA__IS_MULTIBAY = TRUE (IFCBOOLEAN)
    GLOB_CAT_MASTERDATA__SCHEME = "[N] Network" (IFCTEXT)
    GLOB_CAT_MASTERDATA__TYPE = "[C] Component" (IFCTEXT)
  GLOB_CAT_MASTERDATA | properties | on 2 objects (2 IFCELECTRICAPPLIANCE)
    GLOB_CAT_MASTERDATA__GLOB_CAT_CODE = "_RS" (IFCTEXT)
    GLOB_CAT_MASTERDATA__GLOB_CAT_DESC = "ROUTER" (IFCTEXT)
    GLOB_CAT_MASTERDATA__IS_MULTIBAY = TRUE (IFCBOOLEAN)
    GLOB_CAT_MASTERDATA__SCHEME = "[N] Network" (IFCTEXT)
    GLOB_CAT_MASTERDATA__TYPE = "[C] Component" (IFCTEXT)
  GLOB_CAT_MASTERDATA | properties | on 2 objects (2 IFCPROTECTIVEDEVICE)
    GLOB_CAT_MASTERDATA__GLOB_CAT_CODE = "_XQ" (IFCTEXT)
    GLOB_CAT_MASTERDATA__GLOB_CAT_DESC = "SECONDARY SUBSTATIONS LV SWITCHBOARDS" (IFCTEXT)
    GLOB_CAT_MASTERDATA__IS_MULTIBAY = TRUE (IFCBOOLEAN)
    GLOB_CAT_MASTERDATA__SCHEME = "[N] Network" (IFCTEXT)
    GLOB_CAT_MASTERDATA__TYPE = "[C] Component" (IFCTEXT)
  GLOB_CAT_MASTERDATA | properties | on 1 object (1 IFCCOVERING)
    GLOB_CAT_MASTERDATA__GLOB_CAT_CODE = "_XM" (IFCTEXT)
    GLOB_CAT_MASTERDATA__GLOB_CAT_DESC = "PREFABRICATED CONCRETE CABINET" (IFCTEXT)
    GLOB_CAT_MASTERDATA__IS_MULTIBAY = TRUE (IFCBOOLEAN)
    GLOB_CAT_MASTERDATA__SCHEME = "[N] Network" (IFCTEXT)
    GLOB_CAT_MASTERDATA__TYPE = "[C] Component" (IFCTEXT)
  GLOB_CAT_MASTERDATA: 5 more contents on 5 objects not shown
  LOC_TYPE_MASTERDATA | properties | on 3 objects (3 IFCPROTECTIVEDEVICE)
    LOC_TYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DATE = "01-01-2000" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    LOC_TYPE_MASTERDATA__GLOB_CAT_CODE = "_XFMC" (IFCTEXT)
    LOC_TYPE_MASTERDATA__LOC_TYPE_CODE = "DY561/10" (IFCTEXT)
    LOC_TYPE_MASTERDATA__MATERIAL_CODE = "172544" (IFCTEXT)
    LOC_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    LOC_TYPE_MASTERDATA__PARENT_MODEL_ID = "_XFMC" (IFCTEXT)
    LOC_TYPE_MASTERDATA__REVISION_CODE = "02" (IFCTEXT)
    LOC_TYPE_MASTERDATA__SHORT_TEXT = "FUSIBILI MT 24KV 63A L508" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_CODE = "DY561" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_DESC = "CARTUCCIA PER FUSIBILI MT PER INTERNO" (IFCTEXT)
  LOC_TYPE_MASTERDATA | properties | on 3 objects (3 IFCFLOWMETER)
    LOC_TYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DATE = "23-04-2007" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    LOC_TYPE_MASTERDATA__GLOB_CAT_CODE = "_XR" (IFCTEXT)
    LOC_TYPE_MASTERDATA__LOC_TYPE_CODE = "DMI031003" (IFCTEXT)
    LOC_TYPE_MASTERDATA__MATERIAL_CODE = "530002" (IFCTEXT)
    LOC_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    LOC_TYPE_MASTERDATA__PARENT_MODEL_ID = "_XR" (IFCTEXT)
    LOC_TYPE_MASTERDATA__REVISION_CODE = "03" (IFCTEXT)
    LOC_TYPE_MASTERDATA__SHORT_TEXT = "TA APRIBILI CON PRIMARIO PASSANTE 300/5 A" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_CODE = "DMI031003" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_DESC = "TRASFORMATORI DI CORRENTE APRIBILI CON PRIMARIO PASSANTE IN BASSA TENSIONE" (IFCTEXT)
  LOC_TYPE_MASTERDATA | properties | on 1 object (1 IFCCOVERING)
    LOC_TYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DATE = "15-09-2016" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    LOC_TYPE_MASTERDATA__GLOB_CAT_CODE = "_XM" (IFCTEXT)
    LOC_TYPE_MASTERDATA__LOC_TYPE_CODE = "DG2081" (IFCTEXT)
    LOC_TYPE_MASTERDATA__MATERIAL_CODE = "227481" (IFCTEXT)
    LOC_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    LOC_TYPE_MASTERDATA__PARENT_MODEL_ID = "_XM" (IFCTEXT)
    LOC_TYPE_MASTERDATA__REVISION_CODE = "05" (IFCTEXT)
    LOC_TYPE_MASTERDATA__SHORT_TEXT = "Mini Box" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_CODE = "DG2081" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_DESC = "Box in calcestruzzo armato prefabbricato per apparecchiature elettriche per altitudini fino a 1000 metri s.l.m." (IFCTEXT)
  LOC_TYPE_MASTERDATA | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    LOC_TYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DATE = "18-12-2018" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    LOC_TYPE_MASTERDATA__GLOB_CAT_CODE = "_GR" (IFCTEXT)
    LOC_TYPE_MASTERDATA__LOC_TYPE_CODE = "DMIAB000255" (IFCTEXT)
    LOC_TYPE_MASTERDATA__MATERIAL_CODE = "510013" (IFCTEXT)
    LOC_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    LOC_TYPE_MASTERDATA__PARENT_MODEL_ID = "_GR" (IFCTEXT)
    LOC_TYPE_MASTERDATA__REVISION_CODE = "03" (IFCTEXT)
    LOC_TYPE_MASTERDATA__SHORT_TEXT = "Concentratore LVM Low Volt Manager" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_CODE = "DMIAB000255" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_DESC = "Concentratore LVM Low Volt Manager" (IFCTEXT)
  LOC_TYPE_MASTERDATA | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    LOC_TYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DATE = "15-10-2019" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    LOC_TYPE_MASTERDATA__GLOB_CAT_CODE = "_RS" (IFCTEXT)
    LOC_TYPE_MASTERDATA__LOC_TYPE_CODE = "DMIAC000159" (IFCTEXT)
    LOC_TYPE_MASTERDATA__MATERIAL_CODE = "470002" (IFCTEXT)
    LOC_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    LOC_TYPE_MASTERDATA__PARENT_MODEL_ID = "_RS" (IFCTEXT)
    LOC_TYPE_MASTERDATA__REVISION_CODE = "01" (IFCTEXT)
    LOC_TYPE_MASTERDATA__SHORT_TEXT = "4G Router for Low Voltage Manager" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_CODE = "DMIAC000159" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_DESC = "4G Router for Low Voltage Manager" (IFCTEXT)
  LOC_TYPE_MASTERDATA | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    LOC_TYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DATE = "01-01-1900" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    LOC_TYPE_MASTERDATA__GLOB_CAT_CODE = "_RS" (IFCTEXT)
    LOC_TYPE_MASTERDATA__LOC_TYPE_CODE = "IR1101" (IFCTEXT)
    LOC_TYPE_MASTERDATA__MATERIAL_CODE = "480015" (IFCTEXT)
    LOC_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    LOC_TYPE_MASTERDATA__PARENT_MODEL_ID = "_RS" (IFCTEXT)
    LOC_TYPE_MASTERDATA__REVISION_CODE = "00" (IFCTEXT)
    LOC_TYPE_MASTERDATA__SHORT_TEXT = "Cisco IR1101" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_CODE = "IR1101" (IFCTEXT)
  LOC_TYPE_MASTERDATA | properties | on 1 object (1 IFCFLOWMETER)
    LOC_TYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DATE = "28-01-2021" (IFCTEXT)
    LOC_TYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    LOC_TYPE_MASTERDATA__GLOB_CAT_CODE = "_XR" (IFCTEXT)
    LOC_TYPE_MASTERDATA__LOC_TYPE_CODE = "DMIAB000253" (IFCTEXT)
    LOC_TYPE_MASTERDATA__MATERIAL_CODE = "516225" (IFCTEXT)
    LOC_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    LOC_TYPE_MASTERDATA__PARENT_MODEL_ID = "_XR" (IFCTEXT)
    LOC_TYPE_MASTERDATA__REVISION_CODE = "05" (IFCTEXT)
    LOC_TYPE_MASTERDATA__SHORT_TEXT = "GESIS Polyphase 1-20 A CT" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_CODE = "DMIAB000253" (IFCTEXT)
    LOC_TYPE_MASTERDATA__TECH_SPEC_DESC = "POLY PHASE ELECTRONIC METER TIPO GESIS" (IFCTEXT)
  LOC_TYPE_MATGROUP | properties | on 3 objects (3 IFCPROTECTIVEDEVICE)
    LOC_TYPE_MATGROUP__MATGROUP_GLOB = "FEFU0200" (IFCTEXT)
    LOC_TYPE_MATGROUP__MATGROUP_LOC = "T172B" (IFCTEXT)
  LOC_TYPE_MATGROUP | properties | on 3 objects (3 IFCFLOWMETER)
    LOC_TYPE_MATGROUP__MATGROUP_GLOB = "Fetm2200" (IFCTEXT)
    LOC_TYPE_MATGROUP__MATGROUP_LOC = "T531D" (IFCTEXT)
  LOC_TYPE_MATGROUP | properties | on 1 object (1 IFCCOVERING)
    LOC_TYPE_MATGROUP__MATGROUP_LOC = "FECE09" (IFCTEXT)
  LOC_TYPE_MATGROUP | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    LOC_TYPE_MATGROUP__MATGROUP_GLOB = "FTTE0600" (IFCTEXT)
    LOC_TYPE_MATGROUP__MATGROUP_LOC = "T513B" (IFCTEXT)
  LOC_TYPE_MATGROUP | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    LOC_TYPE_MATGROUP__MATGROUP_LOC = "FTTE08" (IFCTEXT)
  LOC_TYPE_MATGROUP | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    LOC_TYPE_MATGROUP__MATGROUP_LOC = "FTTT0800" (IFCTEXT)
  LOC_TYPE_MATGROUP | properties | on 1 object (1 IFCFLOWMETER)
    LOC_TYPE_MATGROUP__MATGROUP_GLOB = "Fscr0900" (IFCTEXT)
    LOC_TYPE_MATGROUP__MATGROUP_LOC = "T512F" (IFCTEXT)
  LOC_TYPE_XM_CT | properties | on 1 object (1 IFCCOVERING)
    LOC_TYPE_XM_CT__XM_ALLOWABLE_OVERLOAD_OF_THE_COVER = "480 daN/mq" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_DIAM_OF_HOLES_FOR_CAB_PASS_POW_STAT = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_DIAM_OF_HOLES_FOR_LV_CABLES_PASSAGE = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_DIAM_OF_HOLES_FOR_MV_CABLES_PASSAGE = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_DIM_OF_ACCESS_OPEN_TO_THE_CELLS_AREA = "1784 mm x 1544 mm (porte)" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_DIM_OF_ACCESS_OPEN_TO_THE_TRANS_AREA = "920 mm x 1600 mm (griglie TR)" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_DOOR_TYPE = "acciaio verniciato" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_EXT_DIM_EMBEDMENT_DEPTH_MAX = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_EXT_DIM_EMBEDMENT_DEPTH_MIN = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_EXT_DIM_LENGTH_MAX = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_EXT_DIM_TOTAL_HEIGHT_MAX = 1950. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_EXT_DIM_TOTAL_HEIGHT_MIN = 1950. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_EXT_DIM_WIDTH_MAX = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_HEIGHT_OG_OPEN_WITH_RESP_EMBED_LEVEL = "170mm - 220 mm" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_INT_DIM_LENGTH_MIN = 2800. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_INT_DIM_TOTAL_USEFUL_LENGTH_MIN = 2800. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_INT_DIM_TOTAL_USEFUL_WIDTH_MIN = 1900. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_INT_DIM_TRANSF_CELL_BOTTOM_MIN = 1900. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_INT_DIM_TRANSF_CELL_WIDTH_MIN = 970. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_INT_DIM_USEFUL_DEPTH_LV_SWIT_AREA_MIN = 870. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_INT_DIM_USEFUL_HEIGHT_TRANSF_CELL = 2300. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_INT_DIM_USEFUL_LENGTH_TRANSF_CELL_MIN = 1900. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_INT_DIM_WIDTH_MIN = 1900. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_XM_CT__XM_LV_SWITCHBOARD_HOLE_DIMENSIONS = "900 mm x 1300 mm (spazio utile in vano BT escluso rack)" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_MAXIMUM_VOLTAGE_NETWORK = 24 (IFCINTEGER)
    LOC_TYPE_XM_CT__XM_MAX_NO_OF_BO_FOR_REM_AND_METER_DA_CON = 1 (IFCINTEGER)
    LOC_TYPE_XM_CT__XM_MAX_NO_OF_LINE_CELLS = 3 (IFCINTEGER)
    LOC_TYPE_XM_CT__XM_MAX_NO_OF_LV_SWITCH_8_OUTPUTS = 2 (IFCINTEGER)
    LOC_TYPE_XM_CT__XM_MAX_NO_OF_TRANSF_CELLS = 1 (IFCINTEGER)
    LOC_TYPE_XM_CT__XM_MAX_NUMBER_OF_REMOTE_CABINETS_MV = 1 (IFCINTEGER)
    LOC_TYPE_XM_CT__XM_MAX_NUMBER_OF_TRANSFORMERS = 1 (IFCINTEGER)
    LOC_TYPE_XM_CT__XM_MAX_NUM_OF_AUX_SERV_SWI_WI_INS_TRANS = 1 (IFCINTEGER)
    LOC_TYPE_XM_CT__XM_MIN_VOLUME_OF_THE_OIL_COLL_TANK = 400. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    LOC_TYPE_XM_CT__XM_MV_CELL_TRENCH_DIMENSIONS = "Fino a 3LE+1T" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_NO_OF_HOLES_FOR_CAB_PASS_POW_STATION = 1 (IFCINTEGER)
    LOC_TYPE_XM_CT__XM_NO_OF_HOLES_FOR_LV_CABLES_PASSAGE = "4" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_NO_OF_HOLES_FOR_MV_CABLES_PASSAGE = "4" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_NO_OF_HOLES_FOR_PASSAGE_EART_CABLES = "No fori, ma zanche metalliche annegate nel cls" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_PERMISSIBLE_MAX_TRANSFORMER_POWER = "fino a 400 kVA" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_PROT_DEGREE_AGAIN_MECH_DAMAGE_ENC = "Porte acciaio in classe 3 UNI EN 1630:2011" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_PROT_DEGREE_ENCL_INC_DOORS_AND_GRIDS = "IP33" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_TYPE_OF_CONSTRUCTION = "Monoblocco o pannelli" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_VENTILATION = "griglie porte - griglieaperture vano TR" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_VERT_EFF_TO_BE_SUPP_BY_THE_FLOOR = "400 daN/mq" (IFCTEXT)
    LOC_TYPE_XM_CT__XM_VERT_EFF_TO_BE_SUPP_BY_THE_FLOOR_TRAN = "TR appoggiato su vasca appoggiata sul terreno" (IFCTEXT)
  OEM_XM_CT | properties | on 1 object (1 IFCCOVERING)
    OEM_XM_CT__XM_OEM_EXT_DIM_EMBEDMENT_DEPTH_MAX = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XM_CT__XM_OEM_EXT_DIM_EMBEDMENT_DEPTH_MIN = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XM_CT__XM_OEM_EXT_DIM_LENGTH_MAX = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XM_CT__XM_OEM_EXT_DIM_WIDTH_MAX = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XM_CT__XM_OEM_INT_DIM_LENGTH_MIN = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XM_CT__XM_OEM_INT_DIM_TRANSF_CELL_BOTTOM_MIN = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XM_CT__XM_OEM_INT_DIM_TRANSF_CELL_WIDTH_MIN = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XM_CT__XM_OEM_INT_DIM_WIDTH_MIN = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  TECH_DETAIL | properties | on 24 objects (24 IFCCABLESEGMENT)
    IfcName = "LV UNDERGROUND CABLE-ED_IT_330304_05" (IFCTEXT)
    TECH_DETAIL__IMAGE_1 = "OEM MODEL.png" (IFCTEXT)
    TECH_DETAIL__IMAGE_2 = "EQUIPMENT.png" (IFCTEXT)
    TECH_DETAIL__LANGUAGE = "IT_EN" (IFCTEXT)
    TECH_DETAIL__LOI_PHASE = "300" (IFCTEXT)
    TECH_DETAIL__MODEL_TYPE_1 = "EQU_MOD" (IFCTEXT)
    TECH_DETAIL__MODEL_TYPE_2 = "EQU_MOD" (IFCTEXT)
    TECH_DETAIL__PARENT_ID_1 = "ED_IT_330304_05" (IFCTEXT)
    TECH_DETAIL__TEMPLATE_1 = "TEMP_OEM" (IFCTEXT)
    TECH_DETAIL__TEMPLATE_2 = "TEMP_OEM_SUBTYPE" (IFCTEXT)
  TECH_DETAIL | properties | on 16 objects (16 IFCCABLEFITTING)
    IfcName = "MORS PERF CTO CAV BT EA0138/3UE-SP_ED_IT_852122_06" (IFCTEXT)
    TECH_DETAIL__IMAGE_1 = "SPARE_PART" (IFCTEXT)
    TECH_DETAIL__LANGUAGE = "IT_EN" (IFCTEXT)
    TECH_DETAIL__LOI_PHASE = "300" (IFCTEXT)
    TECH_DETAIL__MODEL_TYPE_1 = "SP" (IFCTEXT)
    TECH_DETAIL__TEMPLATE_1 = "TEMP_SP" (IFCTEXT)
  TECH_DETAIL | properties | on 15 objects (15 IFCCABLESEGMENT)
    IfcName = "KIT COLLEGAMENTO TRAFO MT-SP_ED_IT_279713_04" (IFCTEXT)
    TECH_DETAIL__IMAGE_1 = "SPARE_PART" (IFCTEXT)
    TECH_DETAIL__LANGUAGE = "IT_EN" (IFCTEXT)
    TECH_DETAIL__LOI_PHASE = "300" (IFCTEXT)
    TECH_DETAIL__MODEL_TYPE_1 = "SP" (IFCTEXT)
    TECH_DETAIL__TEMPLATE_1 = "TEMP_SP" (IFCTEXT)
  TECH_DETAIL | properties | on 11 objects (11 IFCCABLESEGMENT)
    IfcName = "Cavo collegamento UP - DY1051/1-SP_ED_IT_140091_01" (IFCTEXT)
    TECH_DETAIL__IMAGE_1 = "SPARE_PART" (IFCTEXT)
    TECH_DETAIL__LANGUAGE = "IT_EN" (IFCTEXT)
    TECH_DETAIL__LOI_PHASE = "300" (IFCTEXT)
    TECH_DETAIL__MODEL_TYPE_1 = "SP" (IFCTEXT)
    TECH_DETAIL__TEMPLATE_1 = "TEMP_SP" (IFCTEXT)
  TECH_DETAIL | properties | on 10 objects (9 IFCOPENINGELEMENT, 1 IFCCOVERING)
    IfcName = "Basetta per l'installazione del contatore per Bilancio Energia tipo GESIS-SP_ED_IT_280011_02" (IFCTEXT)
    TECH_DETAIL__IMAGE_1 = "SPARE_PART" (IFCTEXT)
    TECH_DETAIL__LANGUAGE = "IT_EN" (IFCTEXT)
    TECH_DETAIL__LOI_PHASE = "300" (IFCTEXT)
    TECH_DETAIL__MODEL_TYPE_1 = "SP" (IFCTEXT)
    TECH_DETAIL__TEMPLATE_1 = "TEMP_SP" (IFCTEXT)
  TECH_DETAIL | properties | on 8 objects (8 IFCCABLEFITTING)
    IfcName = "CAPOCORDA COMPR DIR. 150/13,0BT-SP_ED_IT_210580_01" (IFCTEXT)
    TECH_DETAIL__IMAGE_1 = "SPARE_PART" (IFCTEXT)
    TECH_DETAIL__LANGUAGE = "IT_EN" (IFCTEXT)
    TECH_DETAIL__LOI_PHASE = "300" (IFCTEXT)
    TECH_DETAIL__MODEL_TYPE_1 = "SP" (IFCTEXT)
    TECH_DETAIL__TEMPLATE_1 = "TEMP_SP" (IFCTEXT)
  TECH_DETAIL | properties | on 6 objects (6 IFCCABLECARRIERSEGMENT)
    IfcName = "PASSACAVO STAGNO PER CABINE SECONDARIE-SP_ED_IT_226721_01" (IFCTEXT)
    TECH_DETAIL__IMAGE_1 = "SPARE_PART" (IFCTEXT)
    TECH_DETAIL__LANGUAGE = "IT_EN" (IFCTEXT)
    TECH_DETAIL__LOI_PHASE = "300" (IFCTEXT)
    TECH_DETAIL__MODEL_TYPE_1 = "SP" (IFCTEXT)
    TECH_DETAIL__TEMPLATE_1 = "TEMP_SP" (IFCTEXT)
  TECH_DETAIL | properties | on 4 objects (4 IFCPROTECTIVEDEVICE)
    IfcName = "LV MCCB CIRCUIT BREAKER-ED_IT_131118_00" (IFCTEXT)
    TECH_DETAIL__IMAGE_1 = "OEM MODEL.png" (IFCTEXT)
    TECH_DETAIL__IMAGE_2 = "EQUIPMENT.png" (IFCTEXT)
    TECH_DETAIL__LANGUAGE = "IT_EN" (IFCTEXT)
    TECH_DETAIL__LOI_PHASE = "300" (IFCTEXT)
    TECH_DETAIL__MODEL_TYPE_1 = "EQU_MOD" (IFCTEXT)
    TECH_DETAIL__MODEL_TYPE_2 = "EQU_MOD" (IFCTEXT)
    TECH_DETAIL__PARENT_ID_1 = "ED_IT_131118_00" (IFCTEXT)
    TECH_DETAIL__TEMPLATE_1 = "TEMP_OEM" (IFCTEXT)
    TECH_DETAIL__TEMPLATE_2 = "TEMP_OEM_SUBTYPE" (IFCTEXT)
  TECH_DETAIL: 19 more contents on 27 objects not shown
  GLOB_TYPE_MASTERDATA | properties | on 24 objects (24 IFCCABLESEGMENT)
    GLOB_TYPE_MASTERDATA__DATE = "01-11-2018" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_CAT_CODE = "_XCL" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_TYPE_CODE = "GSC002/008" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__PARENT_MODEL_ID = "_XCL" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__REVISION_CODE = "05" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_CODE = "GSC002" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_DESC = "LOW VOLTAGE UNDERGROUND CABLES WITH RATED VOLTAGE Uo/U(Um) 0,6/1,0 (1,2) kV" (IFCTEXT)
  GLOB_TYPE_MASTERDATA | properties | on 4 objects (4 IFCPROTECTIVEDEVICE)
    GLOB_TYPE_MASTERDATA__ADDENDUM = "N" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__DATE = "20-06-2016" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_CAT_CODE = "_XH" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_TYPE_CODE = "GSCL003/21" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__PARENT_MODEL_ID = "_XH" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__REVISION_CODE = "00" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_CODE = "GSCL003" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_DESC = "AUTOMATIC FOUR-POLE CIRCUIT-BREAKERS WITH 40 A ÷ 630 A RATED CURRENT FOR SECONDARY SUBSTATIONS" (IFCTEXT)
  GLOB_TYPE_MASTERDATA | properties | on 2 objects (2 IFCELECTRICAPPLIANCE)
    GLOB_TYPE_MASTERDATA__DATE = "03-10-2019" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_CAT_CODE = "_MRTU" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_TYPE_CODE = "WM-UP2020 L8 Complete Kit" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__PARENT_MODEL_ID = "_MRTU" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__REVISION_CODE = "02" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_CODE = "GSTR002" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_DESC = "Remote Terminal Unit for MV/LV substation – UP2020 Lite" (IFCTEXT)
  GLOB_TYPE_MASTERDATA | properties | on 2 objects (2 IFCPROTECTIVEDEVICE)
    GLOB_TYPE_MASTERDATA__DATE = "01-07-2020" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_CAT_CODE = "_XQ" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_TYPE_CODE = "GSCL002/01" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__PARENT_MODEL_ID = "_XQ" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__REVISION_CODE = "01" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_CODE = "GSCL002" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_DESC = "LV SWITCHBOARD FOR SECONDARY SUBSTATIONS" (IFCTEXT)
  GLOB_TYPE_MASTERDATA | properties | on 1 object (1 IFCTRANSFORMER)
    GLOB_TYPE_MASTERDATA__DATE = "31-01-2018" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_CAT_CODE = "_MB" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_TYPE_CODE = "GST001/056" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__PARENT_MODEL_ID = "_MB" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__REVISION_CODE = "03" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_CODE = "GST001" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_DESC = "MV/LV TRANSFORMERS" (IFCTEXT)
  GLOB_TYPE_MASTERDATA | properties | on 1 object (1 IFCPROTECTIVEDEVICE)
    GLOB_TYPE_MASTERDATA__DATE = "01-11-2019" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_CAT_CODE = "_XZM" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_TYPE_CODE = "GSCM004/2" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__PARENT_MODEL_ID = "_XZM" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__REVISION_CODE = "00" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_CODE = "GSCM004" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_DESC = "MV RMU CIRCUIT BREAKER" (IFCTEXT)
  GLOB_TYPE_MASTERDATA | properties | on 1 object (1 IFCELECTRICFLOWSTORAGEDEVICE)
    GLOB_TYPE_MASTERDATA__DATE = "18-01-2016" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_CAT_CODE = "_BA" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_TYPE_CODE = "GSCB001/001" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__PARENT_MODEL_ID = "_BA" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__REVISION_CODE = "00" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_CODE = "GSCB001" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_DESC = "ACCUMULATORS VRLA 12V PB FOR POWERING REMOTE-CONTROL DEVICE OF SECONDARY SUBSTATIONS" (IFCTEXT)
  GLOB_TYPE_MASTERDATA | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    GLOB_TYPE_MASTERDATA__DATE = "26-07-2019" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_CAT_CODE = "_RGA" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__GLOB_TYPE_CODE = "GSTP011/RGDM" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__OPER_VERSION = "[S] Yes" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__PARENT_MODEL_ID = "_RGA" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__REVISION_CODE = "01" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_CODE = "GSTP011" (IFCTEXT)
    GLOB_TYPE_MASTERDATA__TECH_SPEC_DESC = "Protection and control device for MV substation – RGDM control unit" (IFCTEXT)
  GLOB_TYPE_MATGROUP | properties | on 24 objects (24 IFCCABLESEGMENT)
    GLOB_TYPE_MATGROUP__MATGROUP_GLOB = "FECA03" (IFCTEXT)
  GLOB_TYPE_MATGROUP | properties | on 4 objects (4 IFCPROTECTIVEDEVICE)
    GLOB_TYPE_MATGROUP__MATGROUP_GLOB = "FEIN11" (IFCTEXT)
  GLOB_TYPE_MATGROUP | properties | on 2 objects (2 IFCELECTRICAPPLIANCE)
    GLOB_TYPE_MATGROUP__MATGROUP_GLOB = "FTTE0501" (IFCTEXT)
  GLOB_TYPE_MATGROUP | properties | on 2 objects (2 IFCPROTECTIVEDEVICE)
    GLOB_TYPE_MATGROUP__MATGROUP_GLOB = "FEQE13" (IFCTEXT)
  GLOB_TYPE_MATGROUP | properties | on 1 object (1 IFCTRANSFORMER)
    GLOB_TYPE_MATGROUP__MATGROUP_GLOB = "FETR1502" (IFCTEXT)
  GLOB_TYPE_MATGROUP | properties | on 1 object (1 IFCPROTECTIVEDEVICE)
    GLOB_TYPE_MATGROUP__MATGROUP_GLOB = "FEQE06" (IFCTEXT)
  GLOB_TYPE_MATGROUP | properties | on 1 object (1 IFCELECTRICFLOWSTORAGEDEVICE)
    GLOB_TYPE_MATGROUP__MATGROUP_GLOB = "FEAP01" (IFCTEXT)
  GLOB_TYPE_MATGROUP | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    GLOB_TYPE_MATGROUP__MATGROUP_GLOB = "FERP0303" (IFCTEXT)
  GLOB_TYPE_MB_CT | properties | on 1 object (1 IFCTRANSFORMER)
    GLOB_TYPE_MB_CT__BLOCKING_DEVICE = 24. (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_MB_CT__BRACKETS_FOR_ARRESTER = "[N] No" (IFCTEXT)
    GLOB_TYPE_MB_CT__BRACKETS_FOR_POLE = "[N] No" (IFCTEXT)
    GLOB_TYPE_MB_CT__CONNECTION_SYMBOL = "[1] Dyn11" (IFCTEXT)
    GLOB_TYPE_MB_CT__COOLING_SYSTEM = "[1] ONAN" (IFCTEXT)
    GLOB_TYPE_MB_CT__FILLING_HOLE_PLUG = "[1] 2” Gas female connection" (IFCTEXT)
    GLOB_TYPE_MB_CT__FREQUENCY = 50 (IFCINTEGER)
    GLOB_TYPE_MB_CT__INSULATING_MATERIAL = "[4] Mineral Oil" (IFCTEXT)
    GLOB_TYPE_MB_CT__LIFTING_DEVICE = "[1] 60" (IFCTEXT)
    GLOB_TYPE_MB_CT__LOAD_LOSS = "[5] 4600" (IFCTEXT)
    GLOB_TYPE_MB_CT__LOSSES_CLASSES = "[5] CkAo" (IFCTEXT)
    GLOB_TYPE_MB_CT__LV_BUSHING_TYPE = "[19] Bus-bar (EN 50387) + insulating protection" (IFCTEXT)
    GLOB_TYPE_MB_CT__LV_INSULATION_LEVEL = "[1] 1.1/--/10" (IFCTEXT)
    GLOB_TYPE_MB_CT__MAX_TOTAL_WEIGHT = 2700. (IFCMASSMEASURE) [KILO GRAM]
    GLOB_TYPE_MB_CT__MIN_INTERAXIS_LIFTING_DEV = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_MB_CT__MV_BUSHING_TYPE = "[10] EN 50180 inside cone plug-in" (IFCTEXT)
    GLOB_TYPE_MB_CT__MV_INSULATION_LEVEL = "[2] 24/125/50" (IFCTEXT)
    GLOB_TYPE_MB_CT__MV_VOLT_REG_TYPE = "[1] DETC" (IFCTEXT)
    GLOB_TYPE_MB_CT__NO_LOAD_LOSS = "[5] 430" (IFCTEXT)
    GLOB_TYPE_MB_CT__OIL_DRAIN_REFERENCE_STANDARD = "[1] EN 50216-4 type C2 (DIN 42551)" (IFCTEXT)
    GLOB_TYPE_MB_CT__OVERALL_DIMENSIONS_HXLXW = "[5] 1850x1600x1030" (IFCTEXT)
    GLOB_TYPE_MB_CT__OVERPRESSURE_VALVE = "[N] No" (IFCTEXT)
    GLOB_TYPE_MB_CT__PAINTING = "[1] Medium" (IFCTEXT)
    GLOB_TYPE_MB_CT__PHASES = "[3] 3P" (IFCTEXT)
    GLOB_TYPE_MB_CT__RATED_LV_FIRST = 0.42 (IFCREAL)
    GLOB_TYPE_MB_CT__RATED_MV_FIRST = 20. (IFCREAL)
    GLOB_TYPE_MB_CT__RATED_POWER = 400. (IFCREAL)
    GLOB_TYPE_MB_CT__SOUND_POWER = 53 (IFCINTEGER)
    GLOB_TYPE_MB_CT__THERMOMETER = "[N] No" (IFCTEXT)
    GLOB_TYPE_MB_CT__VOL_REG = "[1] ±2x2.5%" (IFCTEXT)
    GLOB_TYPE_MB_CT__WHEELS = "[S] Yes" (IFCTEXT)
    GLOB_TYPE_MB_CT__WINDING_MATERIAL = "[3] Copper or Aluminum" (IFCTEXT)
    GLOB_TYPE_MB_CT__ZSC_SHORT_CIRCUIT_VOLTAGE_FROM_UNIF = "[1] 4" (IFCTEXT)
  OEM_MB_CT | properties | on 1 object (1 IFCTRANSFORMER)
    OEM_MB_CT__LENGTH = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_MB_CT__MB_OEM_BLOCKING_DEVICE = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_MB_CT__MB_OEM_MAX_TOTAL_WEIGHT = 0 (IFCINTEGER)
    OEM_MB_CT__MB_OEM_SHORT_CI_SEC_VAL_DOUBLE_SEC_VOLT = 0. (IFCREAL)
    OEM_MB_CT__MB_OEM_SOUND_POWER = 0 (IFCINTEGER)
    OEM_MB_CT__OIL_WEIGHT = 0. (IFCMASSMEASURE) [KILO GRAM]
  SUBTYPE_MASTERDATA | properties | on 24 objects (24 IFCCABLESEGMENT)
    SUBTYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SUBTYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_CAT_CODE = "_XCL" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_TYPE_CODE = "GSC002/008" (IFCTEXT)
    SUBTYPE_MASTERDATA__MATERIAL_CODE = "330304" (IFCTEXT)
    SUBTYPE_MASTERDATA__PARENT_MODEL_ID = "GSC002_008_05" (IFCTEXT)
    SUBTYPE_MASTERDATA__REVISION_CODE = "05" (IFCTEXT)
    SUBTYPE_MASTERDATA__SHORT_TEXT = "LV UNDERGROUND CABLE 1X150 ALUMINUM CONDUCTOR XLPE INSULATION PO JACKET" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_CODE = "GSC002" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_DESC = "LOW VOLTAGE UNDERGROUND CABLES WITH RATED VOLTAGE Uo/U(Um) 0,6/1,0 (1,2) kV" (IFCTEXT)
  SUBTYPE_MASTERDATA | properties | on 4 objects (4 IFCPROTECTIVEDEVICE)
    SUBTYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SUBTYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_CAT_CODE = "_XH" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_TYPE_CODE = "GSCL003/21" (IFCTEXT)
    SUBTYPE_MASTERDATA__MATERIAL_CODE = "131118" (IFCTEXT)
    SUBTYPE_MASTERDATA__PARENT_MODEL_ID = "GSCL003_021_00" (IFCTEXT)
    SUBTYPE_MASTERDATA__REVISION_CODE = "00" (IFCTEXT)
    SUBTYPE_MASTERDATA__SHORT_TEXT = "250/C/25/M" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_CODE = "GSCL003" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_DESC = "AUTOMATIC FOUR-POLE CIRCUIT-BREAKERS WITH 40 A ÷ 630 A RATED CURRENT FOR SECONDARY SUBSTATIONS" (IFCTEXT)
  SUBTYPE_MASTERDATA | properties | on 2 objects (2 IFCELECTRICAPPLIANCE)
    SUBTYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SUBTYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_CAT_CODE = "_MRTU" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_TYPE_CODE = "WM-UP2020 L8 Complete Kit" (IFCTEXT)
    SUBTYPE_MASTERDATA__MATERIAL_CODE = "510021" (IFCTEXT)
    SUBTYPE_MASTERDATA__PARENT_MODEL_ID = "GSTR002_WMUP20L8KIT_02" (IFCTEXT)
    SUBTYPE_MASTERDATA__REVISION_CODE = "02" (IFCTEXT)
    SUBTYPE_MASTERDATA__SHORT_TEXT = "Complete UP2020 Lite kit for Indoor application, mounted in the Wall-mounted indoor cabinet container equipped with UE2020 L8" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_CODE = "GSTR002" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_DESC = "Remote Terminal Unit for MV/LV substation – UP2020 Lite" (IFCTEXT)
  SUBTYPE_MASTERDATA | properties | on 2 objects (2 IFCPROTECTIVEDEVICE)
    SUBTYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SUBTYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_CAT_CODE = "_XQ" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_TYPE_CODE = "GSCL002/01" (IFCTEXT)
    SUBTYPE_MASTERDATA__MATERIAL_CODE = "160125" (IFCTEXT)
    SUBTYPE_MASTERDATA__PARENT_MODEL_ID = "GSCL002_001_01" (IFCTEXT)
    SUBTYPE_MASTERDATA__REVISION_CODE = "01" (IFCTEXT)
    SUBTYPE_MASTERDATA__SHORT_TEXT = "LV SWITCHBOARD FOR SECONDARY SUBSTATIONS" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_CODE = "GSCL002" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_DESC = "LV SWITCHBOARD FOR SECONDARY SUBSTATIONS" (IFCTEXT)
  SUBTYPE_MASTERDATA | properties | on 1 object (1 IFCTRANSFORMER)
    SUBTYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SUBTYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_CAT_CODE = "_MB" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_TYPE_CODE = "GST001/056" (IFCTEXT)
    SUBTYPE_MASTERDATA__MATERIAL_CODE = "113638" (IFCTEXT)
    SUBTYPE_MASTERDATA__PARENT_MODEL_ID = "GST001_056_03" (IFCTEXT)
    SUBTYPE_MASTERDATA__REVISION_CODE = "03" (IFCTEXT)
    SUBTYPE_MASTERDATA__SHORT_TEXT = "MV/LV Transformer 400 KVA 20 / 0,42 kV 3P Dyn11 - Mineral oil" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_CODE = "GST001" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_DESC = "MV/LV TRANSFORMERS" (IFCTEXT)
  SUBTYPE_MASTERDATA | properties | on 1 object (1 IFCPROTECTIVEDEVICE)
    SUBTYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SUBTYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_CAT_CODE = "_XZM" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_TYPE_CODE = "GSCM004/2" (IFCTEXT)
    SUBTYPE_MASTERDATA__MATERIAL_CODE = "140050" (IFCTEXT)
    SUBTYPE_MASTERDATA__PARENT_MODEL_ID = "GSCM004_002_00" (IFCTEXT)
    SUBTYPE_MASTERDATA__REVISION_CODE = "00" (IFCTEXT)
    SUBTYPE_MASTERDATA__SHORT_TEXT = "1T+ 2CBL" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_CODE = "GSCM004" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_DESC = "MV RMU CIRCUIT BREAKER" (IFCTEXT)
  SUBTYPE_MASTERDATA | properties | on 1 object (1 IFCELECTRICFLOWSTORAGEDEVICE)
    SUBTYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SUBTYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_CAT_CODE = "_BA" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_TYPE_CODE = "GSCB001/001" (IFCTEXT)
    SUBTYPE_MASTERDATA__MATERIAL_CODE = "162068" (IFCTEXT)
    SUBTYPE_MASTERDATA__PARENT_MODEL_ID = "GSCB001_001_00" (IFCTEXT)
    SUBTYPE_MASTERDATA__REVISION_CODE = "00" (IFCTEXT)
    SUBTYPE_MASTERDATA__SHORT_TEXT = "ACCUMULATORS VRLA 12V PB" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_CODE = "GSCB001" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_DESC = "ACCUMULATORS VRLA 12V PB FOR POWERING REMOTE-CONTROL DEVICE OF SECONDARY SUBSTATIONS" (IFCTEXT)
  SUBTYPE_MASTERDATA | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    SUBTYPE_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SUBTYPE_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_CAT_CODE = "_RGA" (IFCTEXT)
    SUBTYPE_MASTERDATA__GLOB_TYPE_CODE = "GSTP011/RGDM" (IFCTEXT)
    SUBTYPE_MASTERDATA__MATERIAL_CODE = "160077" (IFCTEXT)
    SUBTYPE_MASTERDATA__PARENT_MODEL_ID = "GSTP011_RGDM_01" (IFCTEXT)
    SUBTYPE_MASTERDATA__REVISION_CODE = "01" (IFCTEXT)
    SUBTYPE_MASTERDATA__SHORT_TEXT = "RGDM" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_CODE = "GSTP011" (IFCTEXT)
    SUBTYPE_MASTERDATA__TECH_SPEC_DESC = "Protection and control device for MV substation – RGDM control unit" (IFCTEXT)
  LOC_TYPE_GR_CT | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    LOC_TYPE_GR_CT__GR_APPLICATION = "1" (IFCTEXT)
    LOC_TYPE_GR_CT__GR_DC_POWER_SUPPLY_FEATURE_EXTERNAL_MODE = "12Vdc @ 12W" (IFCTEXT)
    LOC_TYPE_GR_CT__GR_DIMENSIONS_L_H_P = "198x313x85" (IFCTEXT)
    LOC_TYPE_GR_CT__GR_INSULATION_CATEGORY = 4 (IFCINTEGER)
    LOC_TYPE_GR_CT__GR_INSULATION_VOLTAGE = "5.7" (IFCTEXT)
    LOC_TYPE_GR_CT__GR_IP_GRADE = "41" (IFCTEXT)
    LOC_TYPE_GR_CT__GR_NOMINAL_VOLTAGE_VN = "3x230/400" (IFCTEXT)
    LOC_TYPE_GR_CT__GR_OPERATING_TEMPERATURE = "-25÷ 70" (IFCTEXT)
    LOC_TYPE_GR_CT__GR_RADIO_FREQUENCY_RF_MODEM = 169. (IFCREAL)
    LOC_TYPE_GR_CT__GR_SERIAL_COMMUNICATIONS_PORTS = "RS232 RJ45" (IFCTEXT)
    LOC_TYPE_GR_CT__GR_TERMINAL_CONNECTIONS = "Morsetti 1,5 a 6 mm2" (IFCTEXT)
    LOC_TYPE_GR_CT__GR_TYPE_OF_COMMUNICAT_ON_CENT_SYSTEM_SID = "GSM/GPRS/3G/4G" (IFCTEXT)
    LOC_TYPE_GR_CT__GR_TYPE_OF_COMMUNICAT_ON_THE_METER_SIDE = "PLC/RF" (IFCTEXT)
  SP_MASTERDATA | properties | on 16 objects (16 IFCCABLEFITTING)
    SP_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SP_MASTERDATA__DATE = "21-02-2018" (IFCTEXT)
    SP_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SP_MASTERDATA__MATERIAL_CODE = "852122" (IFCTEXT)
    SP_MASTERDATA__REVISION_CODE = "06" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_CODE = "MPI" (IFCTEXT)
    SP_MASTERDATA__SP_DESCRIPTION = "MORS PERF CTO CAV BT EA0138/3UE" (IFCTEXT)
    SP_MASTERDATA__SUPPLIER = "[E] Enel distribution" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_CODE = "EA0138" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_DESC = "Morsetto a perforazione di isolante per cavi BT" (IFCTEXT)
  SP_MASTERDATA | properties | on 15 objects (15 IFCCABLESEGMENT)
    SP_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SP_MASTERDATA__DATE = "01-11-2006" (IFCTEXT)
    SP_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SP_MASTERDATA__MATERIAL_CODE = "279713" (IFCTEXT)
    SP_MASTERDATA__REVISION_CODE = "04" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_CODE = "CFM" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_DESC = "KIT COLLEGAMENTO TRAFO MT" (IFCTEXT)
    SP_MASTERDATA__SP_DESCRIPTION = "COLL 1P 1TE SC ACI+1TE SC ACE 50MM2 L6M" (IFCTEXT)
    SP_MASTERDATA__SUPPLIER = "[E] Enel distribution" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_CODE = "DJ4448" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_DESC = "COLLEGAMENTI IN CAVO UNIPOLARE MT CONFEZIONATI CON TERMINALI SCONNETTIBILI" (IFCTEXT)
  SP_MASTERDATA | properties | on 11 objects (11 IFCCABLESEGMENT)
    SP_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SP_MASTERDATA__DATE = "09-02-2021" (IFCTEXT)
    SP_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SP_MASTERDATA__MATERIAL_CODE = "140091" (IFCTEXT)
    SP_MASTERDATA__REVISION_CODE = "01" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_CODE = "CUP" (IFCTEXT)
    SP_MASTERDATA__SP_DESCRIPTION = "Cavo collegamento UP - DY1051/1" (IFCTEXT)
    SP_MASTERDATA__SUPPLIER = "[E] Enel distribution" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_CODE = "DY1051" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_DESC = "PRESCRIZIONI PER LA COSTRUZIONE E COLLAUDO DEI CAVI DI COLLEGAMENTO PER IL TELECONTROLLO DELLE MOTORIZZAZIONI IMS E ICS IN CABINA SECONDARIA" (IFCTEXT)
  SP_MASTERDATA | properties | on 10 objects (9 IFCOPENINGELEMENT, 1 IFCCOVERING)
    SP_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SP_MASTERDATA__DATE = "04-09-2012" (IFCTEXT)
    SP_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SP_MASTERDATA__MATERIAL_CODE = "280011" (IFCTEXT)
    SP_MASTERDATA__REVISION_CODE = "02" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_CODE = "BIC" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_DESC = "Basetta per l'installazione del contatore per Bilancio Energia tipo GESIS" (IFCTEXT)
    SP_MASTERDATA__SP_DESCRIPTION = "BASETTA PER L'INSTALL. GET3A GISS GET4S" (IFCTEXT)
    SP_MASTERDATA__SUPPLIER = "[E] Enel distribution" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_CODE = "DMI031071" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_DESC = "BASETTA PER CONTATORI TIPO GET3A - GISS - GET4S" (IFCTEXT)
  SP_MASTERDATA | properties | on 8 objects (8 IFCCABLEFITTING)
    SP_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SP_MASTERDATA__DATE = "01-03-2000" (IFCTEXT)
    SP_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SP_MASTERDATA__MATERIAL_CODE = "210580" (IFCTEXT)
    SP_MASTERDATA__REVISION_CODE = "01" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_CODE = "C1F" (IFCTEXT)
    SP_MASTERDATA__SP_DESCRIPTION = "CAPOCORDA COMPR DIR. 150/13,0BT" (IFCTEXT)
    SP_MASTERDATA__SUPPLIER = "[T] Contractor" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_CODE = "DM4134" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_DESC = "Capocorda diritto a compressione per cavi di bassa tensione" (IFCTEXT)
  SP_MASTERDATA | properties | on 6 objects (6 IFCCABLECARRIERSEGMENT)
    SP_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SP_MASTERDATA__DATE = "15-03-2017" (IFCTEXT)
    SP_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SP_MASTERDATA__MATERIAL_CODE = "226721" (IFCTEXT)
    SP_MASTERDATA__REVISION_CODE = "01" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_CODE = "PSC" (IFCTEXT)
    SP_MASTERDATA__SP_DESCRIPTION = "PASSACAVO STAGNO PER CABINE SECONDARIE" (IFCTEXT)
    SP_MASTERDATA__SUPPLIER = "[E] Enel distribution" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_CODE = "DS920" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_DESC = "Passacavo per cabine secondarie MT/BT" (IFCTEXT)
  SP_MASTERDATA | properties | on 2 objects (2 IFCFURNITURE)
    SP_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SP_MASTERDATA__DATE = "01-12-2002" (IFCTEXT)
    SP_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SP_MASTERDATA__MATERIAL_CODE = "160650" (IFCTEXT)
    SP_MASTERDATA__REVISION_CODE = "03" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_CODE = "LCS" (IFCTEXT)
    SP_MASTERDATA__SP_DESCRIPTION = "TELAIO ACCIAIO SUPPORTO QUADRO BT" (IFCTEXT)
    SP_MASTERDATA__SUPPLIER = "[E] Enel distribution" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_CODE = "DS3055" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_DESC = "TELAIO DI SUPPORTO QUADRO BT DY3009" (IFCTEXT)
  SP_MASTERDATA | properties | on 2 objects (2 IFCCABLEFITTING)
    SP_MASTERDATA__COUNTRY = "[IT] Italy" (IFCTEXT)
    SP_MASTERDATA__DATE = "01-11-2006" (IFCTEXT)
    SP_MASTERDATA__DISTRIBUTION_COMPANY = "[ED] E-Distribuzione" (IFCTEXT)
    SP_MASTERDATA__MATERIAL_CODE = "210562" (IFCTEXT)
    SP_MASTERDATA__REVISION_CODE = "03" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_CODE = "CVS" (IFCTEXT)
    SP_MASTERDATA__SP_CAT_DESC = "CAPOCORDA IN LEGA D'ALLUMINIO CON VITE DI SERRAGGIO" (IFCTEXT)
    SP_MASTERDATA__SP_DESCRIPTION = "CAPOC COMP BIME OCCH COND 150 MMQ" (IFCTEXT)
    SP_MASTERDATA__SUPPLIER = "[T] Contractor" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_CODE = "DM4431" (IFCTEXT)
    SP_MASTERDATA__TECH_SPEC_DESC = "CAPICORDA A COMPRESSIONE BIMETALLICI CON ATTACCO PIATTO AD OCCHIELLO PER CAVI MT CON CONDUTTORI IN ALLUMINIO" (IFCTEXT)
  SP_MASTERDATA: 4 more contents on 4 objects not shown
  LOC_TYPE_XFMC_CT | properties | on 3 objects (3 IFCPROTECTIVEDEVICE)
    LOC_TYPE_XFMC_CT__XFMC_FUSE_LINK_RATED_CURRENT = 63. (IFCREAL)
    LOC_TYPE_XFMC_CT__XFMC_FUSE_LINK_RATED_FREQUENCY = 50 (IFCINTEGER)
    LOC_TYPE_XFMC_CT__XFMC_FUSE_LINK_RATED_MAX_BREAKING_CUR = 16. (IFCREAL)
    LOC_TYPE_XFMC_CT__XFMC_FUSE_LINK_RATED_VOLTAGE = 24. (IFCREAL)
    LOC_TYPE_XFMC_CT__XFMC_FUSE_LINK_TOTAL_LENGHT = 508. (IFCLENGTHMEASURE) [MILLI METRE]
  OEM_XFMC_CT | properties | on 3 objects (3 IFCPROTECTIVEDEVICE)
    OEM_XFMC_CT__XFMC_FUSE_LINK_POWER_DISS_100_RAT_CUR = 0. (IFCREAL)
    OEM_XFMC_CT__XFMC_FUSE_LINK_POWER_DISS_50_RAT_CUR = 0. (IFCREAL)
    OEM_XFMC_CT__XFMC_FUSE_LINK_PROSPECTIVE_CURRENT_I2 = 0. (IFCREAL)
    OEM_XFMC_CT__XFMC_FUSE_LINK_RATED_MIN_BREAKING_CUR = 0. (IFCREAL)
    OEM_XFMC_CT__XFMC_FUSE_LINK_RESIS_AMBIENT_TEMP = 0. (IFCREAL)
    OEM_XFMC_CT__XFMC_FUSE_LINK_SWITCHING_VOLTAGE = 0. (IFCREAL)
  GLOB_TYPE_XZM_CT | properties | on 1 object (1 IFCPROTECTIVEDEVICE)
    GLOB_TYPE_XZM_CT__XZM_ASSEMBLY = "1T+ 2CBL" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UNFIRST_POLE_TO_CLEAR_FAC = "1,3 - 1,5" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UNIT_CLASS = "S1 - C2" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UNIT_ELEC_LECT_REND_CLA = "E2" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UNIT_LINE_DISC_RAT_NOR_CURR = 41.6 (IFCREAL)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UNIT_NUM_MECH_END_CLA = "M2" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UNIT_RATED_NOR_CURR = 630 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UNIT_RAT_CABLE_CHAR_BR_CURR = 31.5 (IFCREAL)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UN_LINE_DISC_EAR_SW_VAL_MECH = "E2" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UN_LINE_DISC_MECH_END_CLASS = 1 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UN_LINE_DISC_RAT_PEAK_WI_CUR = "M1" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UN_LINE_DIS_EAR_SW_PEAK_WI_C = "M1" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UN_LINE_DIS_EAR_SW_RST_WI_CL = 41.6 (IFCREAL)
    GLOB_TYPE_XZM_CT__XZM_CIRC_BR_UN_LINE_DIS_RAT_SHTI_WIT_CUR = 16. (IFCREAL)
    GLOB_TYPE_XZM_CT__XZM_COMMAND_TYPE = "ELECTRIC" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_EXTERNAL_DEGREE_OF_PROTECTION_IK = "IK08" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_EXTERNAL_DEGREE_PROTECTION_IP = "IP3X" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_FUSE_HOLDER = "YES" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_GAS_ENVELOPE_PRESS_SYSTEM = "Sealed" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_INTERNAL_ARC_CLASSIFICATION = "AFL" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_INTERNAL_ARC_TEST_CURRENT = 16 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_INTERNAL_ARC_TEST_CURR_DURATION = 1 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_LOW_POWER_CURR_TRANSF = "YES" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_LOW_POWER_VOLT_TRANSF = "YES" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_MAX_ALTITUDE = 1500000. (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_XZM_CT__XZM_MAX_AMBIENT_AIR_TEMP = 40 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_MAX_POW_CONSUMPTION_AT_FULL_SPEED = 300 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_MAX_PRESSURE_COMPR_GAS = 49.033 (IFCREAL)
    GLOB_TYPE_XZM_CT__XZM_MAX_QUANTITY_OF_SF6_GAS = "< 1.500" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_MIN_AMBIENT_AIR_TEMP = "-15" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_RATED_DURATION_SHORT_CIRCUIT = 1 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_RATED_FREQUENCY = "50/60" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_RATED_LIGHT_IMP_WITH_VOLTAGE = 125 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_RATED_LIGHT_IMP_WITH_VOLTAGE_IS_DIST = 145 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_RATED_NORMAL_CURRENT = 630 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_RATED_PEAK_WITH_CURRENT = 41.6 (IFCREAL)
    GLOB_TYPE_XZM_CT__XZM_RATED_SHORT_DUR_POWER_FREW_WITH_VOLT = 50 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_RATED_SHORT_DUR_POW_FREQ_WITH_IS_DIS = 60 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_RATED_SHORT_TIME_WITH_CURR = 16 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_RATED_SUPPLY_VOLT_AUX_CIRCUIT = 24 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_RATED_VOLTAGE = 24 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_SEISMIC_ACCEPTANCE_CLASS = 2 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_SISMIC_LEVEL = "1-PGA 0,5 g" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_TERMINATIONS_TYPE = "TYPE C BUSHING" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_TIPOLOGY = "Cable lines" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_EA_SW_ES1_ELEC_END_CLASS = "E2" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_EA_SW_ES1_MECH_END_CLASS = "M0" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_EA_SW_ES1_RPEAK_WITH_CURR = 41.6 (IFCREAL)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_EA_SW_ES1_RST_WITH_CURR = 16 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_EA_SW_ES2_ELEC_END_CLASS = "E2" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_EA_SW_ES2_MECH_END_CLASS = "M0" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_EA_SW_ES2_RPEAK_WITH_CURR = 2.5 (IFCREAL)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_EA_SW_ES2_RST_WITH_CURR = 1 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_SW_DISC_ELEC_END_CLASS = "E3" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_SW_DISC_MECH_END_CLASS = "M1" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_SW_DISC_RAT_NOR_CURR = 200 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_SW_DISC_RAT_PEAK_WITH_CUR = 41.6 (IFCREAL)
    GLOB_TYPE_XZM_CT__XZM_TRAN_UN_SW_DISC_RAT_SH_TIME_WITH_CUR = 16 (IFCINTEGER)
    GLOB_TYPE_XZM_CT__XZM_TYPE_OF_ISOLATION = "SF6" (IFCTEXT)
    GLOB_TYPE_XZM_CT__XZM_TYPE_OF_VDS_SYSTEM = "MR" (IFCTEXT)
  OEM_XZM_CT | properties | on 1 object (1 IFCPROTECTIVEDEVICE)
    OEM_XZM_CT__XZM_CLOS_COMAND_ABSOR_MAX_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_CLOS_COMAND_ABSOR_MIN_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_CLOS_COMAND_ABSOR_RATED_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_CLOS_COMAND_TIMING_OP_MAX_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_CLOS_COMAND_TIMING_OP_MIN_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_CLOS_COMAND_TIMING_OP_RATED_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_MINIMUM_PRESSURE = 0. (IFCREAL)
    OEM_XZM_CT__XZM_NOMINAL_PRESSURE = 0. (IFCREAL)
    OEM_XZM_CT__XZM_OPEN_COMAND_ABSOR_MAX_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_OPEN_COMAND_ABSOR_MIN_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_OPEN_COMAND_ABSOR_RATED_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_OPEN_COMAND_TIMING_OP_MAX_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_OPEN_COMAND_TIMING_OP_MIN_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_OPEN_COMAND_TIMING_OP_RATED_AUX_VOLT = 0. (IFCREAL)
    OEM_XZM_CT__XZM_RATED_FILLING_INS_OPER_ATM_AIR_COND = 0. (IFCREAL)
    OEM_XZM_CT__XZM_RESISTANCE_OF_MAIN_CIRCUIT = 0. (IFCREAL)
  GLOB_TYPE_MRTU_CT | properties | on 2 objects (2 IFCELECTRICAPPLIANCE)
    GLOB_TYPE_MRTU_CT__MRTU_ALTITUDE_LEVEL = "[1] 0 ÷ 3000" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_ATMOSPHERIC_PRESSURE = "[1] 67 ÷ 106" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_COMMUNICATION_PROTOCOL_CENTRAL_SYS = "[1] IEC 60870-5-101 / IEC 60870-5-104" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_COMMUNICATION_PROTOCOL_FIELD_DEVICE = "[1] IEC 61850-MQTT" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_CYBER_SECURITY_COMPLIANCE = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_DEPTH = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_MRTU_CT__MRTU_LENGTH = 720. (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_MRTU_CT__MRTU_NUMBER_OF_CHANNELS = 8 (IFCINTEGER)
    GLOB_TYPE_MRTU_CT__MRTU_OPERATING_TEMPERATURE = "[-0.35714285714285715]" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_OUTDOOR_BOX_MATERIAL = "[3] NA" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_OUT_BOX_DOOR_WITH_A_PADLOCK = "[2] NA" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_PSBC_AC_SOURCE = "[1] 100-230" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_PSBC_DC_OUTPUT = 24 (IFCINTEGER)
    GLOB_TYPE_MRTU_CT__MRTU_RELATIVE_HUMIDITY = "[1] 0 ÷ +95" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_REM_ACC_TO_LOG_WITH_104_FILE_TRAN = "[2] NA" (IFCTEXT)
    GLOB_TYPE_MRTU_CT__MRTU_RTU_DC_SOURCE = 24 (IFCINTEGER)
    GLOB_TYPE_MRTU_CT__MRTU_WIDTH = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  GLOB_TYPE_BA_CT | properties | on 1 object (1 IFCELECTRICFLOWSTORAGEDEVICE)
    GLOB_TYPE_BA_CT__BA_ACCUM_LIFE_EXPECTANCY_MIN = 12. (IFCREAL)
    GLOB_TYPE_BA_CT__BA_ACCUM_MAX_LENGTH_HEIGHT_DEPT = "[3] 250/170/175" (IFCTEXT)
    GLOB_TYPE_BA_CT__BA_ACCUM_RATED_CAPACITY = 25. (IFCREAL)
    GLOB_TYPE_BA_CT__BA_CONNECTOR_PERFORMANCE = 0.6 (IFCREAL)
    GLOB_TYPE_BA_CT__BA_FLAMABILTY_RATING_OF_MATERIALS = "V-0" (IFCTEXT)
    GLOB_TYPE_BA_CT__BA_MAXIMUM_ALTITUDE = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_BA_CT__BA_MAXIMUM_ATMOSPHERIC_PRESSURE = 106. (IFCREAL)
    GLOB_TYPE_BA_CT__BA_MAXIMUM_OPERATING_TEMPERATURE = 50. (IFCREAL)
    GLOB_TYPE_BA_CT__BA_MAXIMUM_RELATIVE_HUNIDITY = 95 (IFCINTEGER)
    GLOB_TYPE_BA_CT__BA_MAXIMUM_WEIGHT = 15. (IFCMASSMEASURE) [KILO GRAM]
    GLOB_TYPE_BA_CT__BA_MAX_STORAGE_TRANSPORT_TEMPERATURE = 70. (IFCREAL)
    GLOB_TYPE_BA_CT__BA_MINIMUM_ACCUM_RATED_CAPACITY_1 = "76% of C10" (IFCTEXT)
    GLOB_TYPE_BA_CT__BA_MINIMUM_ACCUM_RATED_CAPACITY_2 = "78% of C10" (IFCTEXT)
    GLOB_TYPE_BA_CT__BA_MINIMUM_ATMOSPHERIC_PRESSURE = 70. (IFCREAL)
    GLOB_TYPE_BA_CT__BA_MINIMUM_OPERATING_TEMPERATURE = -20. (IFCREAL)
    GLOB_TYPE_BA_CT__BA_MIN_STORAGE_TRANSPORT_TEMPERATURE = -25. (IFCREAL)
    GLOB_TYPE_BA_CT__BA_RATED_VOLTAGE = 12. (IFCREAL)
    GLOB_TYPE_BA_CT__BA_VOLTAGE_EQUALIZING_CHARGE = "2,26 ÷2,30" (IFCTEXT)
  SUBTYPE_BA_CT | properties | on 1 object (1 IFCELECTRICFLOWSTORAGEDEVICE)
    SUBTYPE_BA_CT__BA_MAXIMUM_ALTITUDE = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
  GLOB_TYPE_RGA_CT | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    GLOB_TYPE_RGA_CT__RGA_ALTITUDE_LEVEL = "[1] 0 ÷ 3000" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_ATMOSPHERIC_PRESSURE = "[1] 67 ÷ 106" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_COMMUNICATION_PROTOCOL = "[1] IEC 61850" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_CURR_MEAS_CIRC = "[1] IA, IB, IC" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_CURR_MEAS_CIRC_CALIBRATION_VIA_SW = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_CURR_MEAS_CIRC_MEASUREMENT_RANGE = "[1] 0 ÷ 8800" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_CURR_MEAS_CIRC_MEAS_AVAIL_VIA_ANAL = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_CURR_MEAS_CIRC_MIN_ACC_REQUIRED = 0.2 (IFCREAL)
    GLOB_TYPE_RGA_CT__RGA_CURR_MEAS_CIRC_NOM_CURR_RANGE = "[1] 0 ÷ 500" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_CURR_MEAS_CIRC_PIM_SEC_RATES_ALLOW = "[1] 1000A/31mV 1000A/100mV 1000A/300mV" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_CURR_MEAS_CIRC_RELATION_IPRIM_ISEC = "[1] Linear, derivative" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_CURR_VOLT_SENS_INTERFACES = "[1] 7 (3 for GSCT005 sensors, 3 for older versions, 1 for busbar voltage)" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_CURR_VOLT_SENS_INTERFACE_TYPE = "[1] RJ45" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_CYBER_SECURITY_COMPLIANCE = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_DC_CA_MAX_COMPONENT = 10 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_DC_POLARITY_INVERSION_PROTECTED = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_DC_SOURCE = 24 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_DEPTH = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_RGA_CT__RGA_DFR_NUMB_OF_ANALOG_CHANNELS = "[1] > 8" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_DFR_NUMB_OF_DIGITAL_CHANNELS = "[1] >= 100" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_DFR_RECORDS_STORAGE = "" - Minimum 48 hours with loss of power supply - Storage capacity: 1000s - Pre-fault recording (0 -2000 ms, duration configurable via software) - Recording of the disturbance event (duration configurable via software [0 ÷ 70 s]) - Post-trigger recording (duration configurable via software [0 ÷ 2000 ms]) - All the starts/trips of the FdPs, digital I/O, logic I/O must be configurable as trigger events."" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_DIGIT_FAULT_REC = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_DIGIT_FAULT_REC_DOWNLOAD_VIA_COM_PO = "[1] Web server, SFTP" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_DIGIT_FAULT_REC_FILE_FORMAT = "[1] COMTRADE" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_DIGIT_FAULT_REC_MAX_SAMP_RATE = 2.5 (IFCREAL)
    GLOB_TYPE_RGA_CT__RGA_DISPLAY = "[1] Graphic LCD display with a resolution capable to display: · Fault events · Inversion activated · Voltage presesence · Device anomaly · Measurements · Configuration settings · Date/hour · SNTP status · Ethernet configuration · RGDM serial number" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_ENCLOSURE_MATERIAL = "[1] Steel or aluminum" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_ETHERN_COMM_PORT_100_BASE_INTERFACE = 1 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_ETHERN_COMM_PORT_IEC61850_SERVICES = "[1] MMS, Goose, File Transfer" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_ETHERN_COMM_PORT_OTHER_SERVICES = "[1] web server, SNTP, SSH" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_ETHERN_COMM_PORT_PROTOCOLS = "[1] TCP, IP-UDP" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_EVENT_LOGS_DOWNLOAD_VIA_CONFIG_SW = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_EVENT_LOGS_DOWNLOAD_VIA_REMOTE_CONN = "[1] SFTP" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_EVENT_LOGS_EVENT_REG_LOG_CAPACITY = "[1] >= 1024" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_EVENT_LOGS_FAULT_REG_LOG_CAPACITY = "[1] >= 200" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_EVENT_LOGS_MEAS_REG_LOG_CAPACITY = "[1] >= 4320" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_EVENT_LOGS_TYPE_OF_SIGNALS_RECORDED = "[1] All (inputs, outputs, plc, internal, protection, etc)" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_FRONTAL_PANEL_ELEMENTS = "[1] CB open/close push buttons Naviagtio buttons Rotating selector for activating/deactivating reclosing Display" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_IP_GRADE = "[1] IP30" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_LEDS = 10 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_LEDS_DEFINED_BY_USER = 8 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_LEDS_DEVICE_STATE = 2 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_LENGTH = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_RGA_CT__RGA_MAX_POWER_CONSUMPTION = 15 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_MTBF = 30 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_MTTR = 3 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_OPERATING_TEMPERATURE = "[1] -25 ÷ +70" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PLC = "[1] Yes, using digital and analog variables" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PLC_PROGRAMMING = "[1] CFC, ST, LD language" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_BREAKER_FAIL_FUNCT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_BROK_COND_DETECT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_COLD_LOAD_PICK_UP = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_CONTR_TRIP_TIME_FUNC = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_CYCLE_DIR_CHECK_FUN = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_DG_MANAGEMENT_FUNCT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_DIRECT_NON_DIR_OVERC = "[1] 4 stages" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_DIRE_MAX_ACT_POW_PRO = "[1] 1 stage" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_DIR_EARTH_OVERCU_PRO = "[1] 4 stages" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_FRL_AUT_FUNCT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_FSL_AUT_FUNCT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_HOMOPOL_OVERVOL_PRO = "[1] 2 stages" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_HOT_LINE_TAG_FUNCT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_INRUSH_FUNCTION = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_OPEN_PHASE_PROTECT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_OVERVOL_NEG_SEQ_PROT = "[1] 1 stage" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_OVERVOL_PROT_FUNCT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_RECLOSER_FUNCT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_RES_OVERCURR_PROT = "[1] 3 stages" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_SECT_AUTOM_FUNCTION = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_SFS_AUT_FUNCT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_SKIP_SHOT_FUNCTION = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_SYNCHRO_CHECK_FUNC = "[1] N.A." (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_UPG_FUNCT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_VOLTAGE_DETECTION = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_VOLTAGE_SENS_SUPERV = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT_ZONE_SEQ_COORD_FUNC = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_PROT_AUT_FUNCT__FREQ_PROT_FUNCT = "[1] 2 stages" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_RELATIVE_HUMIDITY = "[1] 0 ÷ 95" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_RJ45_PIN_ASSIGNEMENT_CONFIGURATION = "[1] For GSCT005 Sensors: Pins according to IEC61869-10/IEC61869-11" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_RTU_CONN_CABLE_CURR_CARRY_CAPACITY = 13 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_RTU_CONN_CABLE_ISOLATION = "[1] PVC - R2" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_RTU_CONN_CABLE_LENGTH = "[1] 9 (indoor)1,5 (outdoor)" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_RTU_CONN_CABLE_PINS_IDENTIFIC_REQ = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_RTU_CONN_CABLE_RATED_VOLTAGE = 24 (IFCINTEGER)
    GLOB_TYPE_RGA_CT__RGA_RTU_CONN_CABLE_STRUCTURE = "[1] 9x1mm2" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_SW_CAPAB_CURR_VOLT_MEAS_AUTOCAL = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_SW_CAPAB_DIGITAL_OUTPUT_TEST = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_SW_CAPAB_EVENT_RECORDER_DOWNLOAD = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_SW_CAPAB_FW_UPGRADE = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_SW_CAPAB_IEC61850_CONFIG_FILE_MANAG = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_SW_CAPAB_IEC61850_SET_AND_MMSS_CONF = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_SW_CAPAB_MEAS_MONITORING = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_SW_CAPAB_PROTECTION_PARAM_SETT = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_SW_CAPAB_SELF_DIAGNOSIS = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_SYNCHRONIZATION_PROTOCOL = "[1] NTP" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_TERMINAL_BOARDS_CABLE_WIRED_SECTION = 2.5 (IFCAREAMEASURE) [SQUARE_METRE]
    GLOB_TYPE_RGA_CT__RGA_TERM_BOARDS_PINS_IDENTIFICATION_REQ = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_TERM_BOARDS_REMOVABLE_TERM_BOARD = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_TYPE_OF_SENSORS = "[1] GSCT005 Compliant" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_VOLT_MEAS_CIRC = "[1] VA, VB, VC, Vsyn" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_VOLT_MEAS_CIRCMEAS_AVAIL_VIA_ANAL = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_VOLT_MEAS_CIRC_CALIBRATION_VIA_SW = "[1] Yes" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_VOLT_MEAS_CIRC_CONFIG_RATIO = "[1] 10000/1 (MV)230/1 (LV)" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_VOLT_MEAS_CIRC_MIN_ACC_REQUIRED = 0.2 (IFCREAL)
    GLOB_TYPE_RGA_CT__RGA_VOLT_MEAS_CIRC_SEC_VOLT_RANGE_VALUE = "[1] 0 ÷ 3,96" (IFCTEXT)
    GLOB_TYPE_RGA_CT__RGA_WIDTH = 300. (IFCLENGTHMEASURE) [MILLI METRE]
  SUBTYPE_RGA_CT | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    SUBTYPE_RGA_CT__RGA_DC_SOURCE_OPERATING_RANGE = "[1] N.A." (IFCTEXT)
    SUBTYPE_RGA_CT__RGA_PROT_AUT_FUNCT_FPI_ACOR_TO_FUNC_END = "[1] NA" (IFCTEXT)
  GLOB_TYPE_XCL_CT | properties | on 24 objects (24 IFCCABLESEGMENT)
    GLOB_TYPE_XCL_CT__INSULATION_COLOR = "[2] Natural (colorless)" (IFCTEXT)
    GLOB_TYPE_XCL_CT__INSULATION_MATERIAL = "[19] XLPE" (IFCTEXT)
    GLOB_TYPE_XCL_CT__INSULATION_MINIMUM_THICKNESS_XCL = 1.16 (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_XCL_CT__INSULATION_NOMINAL_THICKNESS_XCL = 1.4 (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_XCL_CT__MAXIMUM_CONDUCTOR_DIAMETER = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_XCL_CT__MAXIMUM_RESISTANCE_OF_CONDUCTOR = 0.206 (IFCREAL)
    GLOB_TYPE_XCL_CT__MINIMUM_CONDUCTOR_DIAMETER = 13.7 (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_XCL_CT__MINIMUM_NUMBER_WIRES_CONDUCTOR = 15 (IFCINTEGER)
    GLOB_TYPE_XCL_CT__RATED_VOLTAGE_XCL = "[2] 0,6 / 1 kV" (IFCTEXT)
    GLOB_TYPE_XCL_CT__SHEATH_COLOR = "[2] BLACK" (IFCTEXT)
    GLOB_TYPE_XCL_CT__SHEATH_MATERIAL = "[7] PO" (IFCTEXT)
    GLOB_TYPE_XCL_CT__SHEATH_MINIMUM_THICKNESS_XCL = 1.09 (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_XCL_CT__SHEATH_NOMINAL_THICKNESS_XCL = 1.4 (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_XCL_CT__STANDING_TYPE_CONDUCTOR = "[1] Circular compacted class 2" (IFCTEXT)
    GLOB_TYPE_XCL_CT__TYPE_OF_CABLE = "[1] I" (IFCTEXT)
    GLOB_TYPE_XCL_CT__XCL_CONDUCTOR_NOMINAL_CROSS_SECTION = "[8] 1X150" (IFCTEXT)
  SUBTYPE_XCL_CT | properties | on 24 objects (24 IFCCABLESEGMENT)
    SUBTYPE_XCL_CT__CONDUCTOR_MATERIAL_XC = "[1] ALUMINUM" (IFCTEXT)
  LOC_TYPE_RS_CT | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    LOC_TYPE_RS_CT__RS_ALTITUDE_LEVEL = "N/A" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_DEPTH = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_RS_CT__RS_HEIGHT = 320. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_RS_CT__RS_IP_RATING = "IP22 for the connectors area IP51 for the case/cabinet area IP54 for the SIM card space" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_OPERATING_TEMPERATURE = "-25 ÷ +55" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_POWER_CONSUMPTION_MAX = "23" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_POWER_SUPPLY = "12 ÷ 28,8 DC" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_RELATIVE_HUMIDITY = "N/A" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_WEIGHT = 1.2 (IFCMASSMEASURE) [KILO GRAM]
    LOC_TYPE_RS_CT__RS_WIDTH = 200. (IFCLENGTHMEASURE) [MILLI METRE]
  LOC_TYPE_RS_CT | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    LOC_TYPE_RS_CT__RS_ALTITUDE_LEVEL = "0 ÷ 4200" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_DEPTH = 124.9 (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_RS_CT__RS_HEIGHT = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    LOC_TYPE_RS_CT__RS_IP_RATING = "IP30" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_OPERATING_TEMPERATURE = "-40 ÷ +75" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_POWER_CONSUMPTION_MAX = "13" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_POWER_SUPPLY = "9,6 ÷ 60 DC" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_RELATIVE_HUMIDITY = "5 ÷ +95" (IFCTEXT)
    LOC_TYPE_RS_CT__RS_WEIGHT = 1.02 (IFCMASSMEASURE) [KILO GRAM]
    LOC_TYPE_RS_CT__RS_WIDTH = 132.5 (IFCLENGTHMEASURE) [MILLI METRE]
  OEM_RS_CT | properties | on 2 objects (2 IFCELECTRICAPPLIANCE)
    OEM_RS_CT__RS_OEM_DEPTH = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_RS_CT__RS_OEM_HEIGHT = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_RS_CT__RS_OEM_POWER_CONSUMPTION_MAX = 0. (IFCREAL)
    OEM_RS_CT__RS_OEM_WEIGHT = 0. (IFCMASSMEASURE) [KILO GRAM]
    OEM_RS_CT__RS_OEM_WIDTH = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  OEM_RS_CT_IT | properties | on 2 objects (2 IFCELECTRICAPPLIANCE)
    OEM_RS_CT_IT__RS_OEM_NUM_CHANNELS = 0. (IFCREAL)
    OEM_RS_CT_IT__RS_OEM_SUPPLY_VOLTAGE = 0. (IFCREAL)
  LOC_TYPE_XR_CT | properties | on 3 objects (3 IFCFLOWMETER)
    LOC_TYPE_XR_CT__APPLICATION = "[1] Outdoor" (IFCTEXT)
    LOC_TYPE_XR_CT__CONSTRUCTION_TYPE_XR = "[4] Split core type current transformer (ring primary type)" (IFCTEXT)
    LOC_TYPE_XR_CT__FREQUENCY = 50 (IFCINTEGER)
    LOC_TYPE_XR_CT__INTERNAL_EXTERNAL_DIAMETER = "[2] 60/150" (IFCTEXT)
    LOC_TYPE_XR_CT__NOMINAL_CURRENT_RATIO = "[1] 300/5 A/A" (IFCTEXT)
    LOC_TYPE_XR_CT__PRECISION_CLASS = "[1] 0.55" (IFCTEXT)
    LOC_TYPE_XR_CT__PRIMARY_CURRENT = 300 (IFCINTEGER)
    LOC_TYPE_XR_CT__SECONDARY_CURRENT = 5 (IFCINTEGER)
    LOC_TYPE_XR_CT__SHORT_CIRCUIT_CURRENT_XR = 12.5 (IFCREAL)
    LOC_TYPE_XR_CT__XR_MAX_CURRENT = 1200 (IFCINTEGER)
    LOC_TYPE_XR_CT__XR_MAX_REFERENCE_VOLT_FOR_INS = 0.72 (IFCREAL)
    LOC_TYPE_XR_CT__XR_OPERATING_TEMPERATURE = "-25 ÷ 70" (IFCTEXT)
    LOC_TYPE_XR_CT__XR_OVERLOADABILITY = "4" (IFCTEXT)
    LOC_TYPE_XR_CT__XR_TRANSFORMATION_CONSTANT = 60 (IFCINTEGER)
    LOC_TYPE_XR_CT__XR_VA_PERFORMANCE = "2.5" (IFCTEXT)
  LOC_TYPE_XR_CT | properties | on 1 object (1 IFCFLOWMETER)
    LOC_TYPE_XR_CT__APPLICATION = "[2] Indoor" (IFCTEXT)
    LOC_TYPE_XR_CT__CONSTRUCTION_TYPE_XR = "[5] Semi-direct insertion" (IFCTEXT)
    LOC_TYPE_XR_CT__FREQUENCY = 50 (IFCINTEGER)
    LOC_TYPE_XR_CT__PRECISION_CLASS = "[2] ACTIVE class B REACTIVE class 2" (IFCTEXT)
    LOC_TYPE_XR_CT__SHORT_CIRCUIT_CURRENT_XR = 6. (IFCREAL)
    LOC_TYPE_XR_CT__XR_CONNECTION_TYPE = "INNESTO RAPIDO CON SPINOTTI" (IFCTEXT)
    LOC_TYPE_XR_CT__XR_DIMENSIONS = "195,5x296x107" (IFCTEXT)
    LOC_TYPE_XR_CT__XR_MAX_CURRENT = 20 (IFCINTEGER)
    LOC_TYPE_XR_CT__XR_MAX_REFERENCE_VOLT_FOR_INS = 0.72 (IFCREAL)
    LOC_TYPE_XR_CT__XR_OPERATING_TEMPERATURE = "-25 ÷ 70" (IFCTEXT)
    LOC_TYPE_XR_CT__XR_RATED_CURRENT = 1 (IFCINTEGER)
    LOC_TYPE_XR_CT__XR_VOLTAGE = "3X230/400" (IFCTEXT)
  OEM_XR_CT | properties | on 4 objects (4 IFCFLOWMETER)
    OEM_XR_CT__HEIGHT = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XR_CT__LENGTH = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XR_CT__WIDTH = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  GLOB_TYPE_XQ_CT | properties | on 2 objects (2 IFCPROTECTIVEDEVICE)
    GLOB_TYPE_XQ_CT__XQ_DIMENSIONS = "410x250x650" (IFCTEXT)
    GLOB_TYPE_XQ_CT__XQ_EXTERNAL_DEGREE_OF_PROTECTION_IK = "IK08" (IFCTEXT)
    GLOB_TYPE_XQ_CT__XQ_EXTERNAL_DEGREE_OF_PROTECTION_IP = "IP3X" (IFCTEXT)
    GLOB_TYPE_XQ_CT__XQ_RATED_FREQUENCY = "50/60" (IFCTEXT)
    GLOB_TYPE_XQ_CT__XQ_RATED_LIGHT_IMP_WITH_VOLTAGE = 20 (IFCINTEGER)
    GLOB_TYPE_XQ_CT__XQ_RATED_POW_FREQ_WITH_VOLTAGE = 10 (IFCINTEGER)
    GLOB_TYPE_XQ_CT__XQ_RATED_SHORT_TIME_WITH_CURRENT = 16 (IFCINTEGER)
    GLOB_TYPE_XQ_CT__XQ_RATED_VOLTAGE = 400 (IFCINTEGER)
  SUBTYPE_XQ_CT | properties | on 2 objects (2 IFCPROTECTIVEDEVICE)
    SUBTYPE_XQ_CT__XQ_RATED_NORMAL_CURRENT = 650 (IFCINTEGER)
  GLOB_TYPE_XH_CT | properties | on 4 objects (4 IFCPROTECTIVEDEVICE)
    GLOB_TYPE_XH_CT__CONVENTIONAL_NONTRIPPING_CURRENT = "[1] 1,05 Ith" (IFCTEXT)
    GLOB_TYPE_XH_CT__CONVENTIONAL_TRIPPING_CURRENT = "[1] 1,30 Ith" (IFCTEXT)
    GLOB_TYPE_XH_CT__CONV_NEUTRAL_NONTRIPPING_CURRENT = "[1] 1,05 Ith" (IFCTEXT)
    GLOB_TYPE_XH_CT__CONV_NEUTRAL_TRIPPING_CURRENT = "[1] 1,30 Ith" (IFCTEXT)
    GLOB_TYPE_XH_CT__CURRENT_PHASE_MAGNETIC = "[1] 1250" (IFCTEXT)
    GLOB_TYPE_XH_CT__CURRENT_PHASE_TERMAL = "[1] 250" (IFCTEXT)
    GLOB_TYPE_XH_CT__INSTALLATION_TYPE = "[3] Secondary substations" (IFCTEXT)
    GLOB_TYPE_XH_CT__IP_CODE = "[1] IP3X" (IFCTEXT)
    GLOB_TYPE_XH_CT__LOWER_LIMIT_AMBIENT_TEMPERATURE = "[1] -20" (IFCTEXT)
    GLOB_TYPE_XH_CT__MOTOR_DRIVEN = "[2] Electric" (IFCTEXT)
    GLOB_TYPE_XH_CT__NEUTRAL = "[2] Uninterrupted" (IFCTEXT)
    GLOB_TYPE_XH_CT__NEUTRAL_MAGNETIC_RELEASE_CURRENT_SET = 800 (IFCINTEGER)
    GLOB_TYPE_XH_CT__NEUTRAL_THERMAL_RELEASE = "[2] 100" (IFCTEXT)
    GLOB_TYPE_XH_CT__RATED_IMPULSE_VOLTAGE = 8 (IFCINTEGER)
    GLOB_TYPE_XH_CT__RATED_INSULATION_VOLTAGE = 690 (IFCINTEGER)
    GLOB_TYPE_XH_CT__RATED_SHORT_CIRCUIT_BREAKING_CAPACITY = 25 (IFCINTEGER)
    GLOB_TYPE_XH_CT__RATED_UNINTERRUPTED_CURRENT = 250 (IFCINTEGER)
    GLOB_TYPE_XH_CT__RATED_VOLTAGE_XH = 400 (IFCINTEGER)
    GLOB_TYPE_XH_CT__SERVICE = "[1] Uninterrupted" (IFCTEXT)
    GLOB_TYPE_XH_CT__UPPER_LIMIT_AMBIENT_TEMPERATURE = 40 (IFCINTEGER)
    GLOB_TYPE_XH_CT__UTILIZATION_CATEGORY = "[A]" (IFCTEXT)
    GLOB_TYPE_XH_CT__XH_EXT_DEGREE_PROT_IP_OF_MOTORIZATION = "IP4X" (IFCTEXT)
    GLOB_TYPE_XH_CT__XH_FREQUENCY = "[1] 50/60" (IFCTEXT)
    GLOB_TYPE_XH_CT__XH_MAX_ALTITUDE = 2000000. (IFCLENGTHMEASURE) [MILLI METRE]
    GLOB_TYPE_XH_CT__XH_MAX_OPERATION_TIME_OF_MOTORIZATION = 5. (IFCREAL)
    GLOB_TYPE_XH_CT__XH_MAX_PERMIS_ABS_CURR_OF_MOTORIZATION = 13. (IFCREAL)
    GLOB_TYPE_XH_CT__XH_NEUT_MAGN_REL_BREAK_TIME_FOR_TRIP_CUR = "≤15" (IFCTEXT)
    GLOB_TYPE_XH_CT__XH_NEUT_MAGN_REL_TRIP_CURR_PRECISION = "±20" (IFCTEXT)
    GLOB_TYPE_XH_CT__XH_NEUT_THER_REL_MAX_BREAK_TIME = 8. (IFCREAL)
    GLOB_TYPE_XH_CT__XH_PHASE_MAGN_REL_BREAK_TIME_TRIP_CUR = "≤15" (IFCTEXT)
    GLOB_TYPE_XH_CT__XH_PHASE_MAGN_REL_TRIP_CURR_PRECISION = "±20" (IFCTEXT)
    GLOB_TYPE_XH_CT__XH_PHASE_THER_REL_MAX_BREAK_TIME = 12. (IFCREAL)
    GLOB_TYPE_XH_CT__XH_RATED_SUPPLY_VOLT_AUX_AND_CONTR_CIRC = 24. (IFCREAL)
    GLOB_TYPE_XH_CT__XH_SEISMIC_LEVEL = "NO" (IFCTEXT)
    GLOB_TYPE_XH_CT__XH_VDS_PRESSENCE = TRUE (IFCBOOLEAN)
  OEM_XH_CT | properties | on 4 objects (4 IFCPROTECTIVEDEVICE)
    OEM_XH_CT__HEIGHT = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XH_CT__LENGTH = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XH_CT__WIDTH = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    OEM_XH_CT__XH_CIRC_BR_CLOS_ABS_MAX_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_ABS_MAX_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_ABS_MAX_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_ABS_MIN_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_ABS_MIN_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_ABS_MIN_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_ABS_RAT_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_ABS_RAT_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_ABS_RAT_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_TIM_OP_MAX_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_TIM_OP_MAX_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_TIM_OP_MAX_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_TIM_OP_MIN_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_TIM_OP_MIN_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_TIM_OP_MIN_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_TIM_OP_RAT_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_TIM_OP_RAT_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_CLOS_TIM_OP_RAT_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_ABS_MAX_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_ABS_MAX_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_ABS_MAX_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_ABS_MIN_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_ABS_MIN_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_ABS_MIN_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_ABS_RAT_AUX_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_ABS_RAT_AUX_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_ABS_RAT_AUX_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_TIM_OP_MAX_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_TIM_OP_MAX_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_TIM_OP_MAX_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_TIM_OP_MIN_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_TIM_OP_MIN_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_TIM_OP_MIN_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_TIM_OP_RAT_AU_VOLT_AT_20 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_TIM_OP_RAT_AU_VOLT_AT_40 = 0. (IFCREAL)
    OEM_XH_CT__XH_CIRC_BR_OPEN_TIM_OP_RAT_AU_VOLT_AT_5 = 0. (IFCREAL)
    OEM_XH_CT__XH_OVERALL_DIM_X_Y_Z = 0. (IFCREAL)